CSIM Code Reference Manual Version 4

by Bruce P. Briegleb^1

May 13, 2002 1

1National Center for Atmospheric Research, PO Box 3000, Boulder CO 80307 (NCAR is sponsored by the National Science Foundation)

Contents

1 Introduction 6

2 Overview of CSIM4 Code 6 2.1 Calling Tree . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8

3 Data Structures 10 3.1 Horizontal . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10 3.2 Category . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10 3.3 Vertical . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11

4 Module Descriptions 11 4.1 Fortran: Module Interface icemodel - main ice model program (Source File: ice.F) . . . . . . 11 4.2 Fortran: Module Interface ice albedo - snow and ice albedo parameterization (Source File:

ice albedo.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12 4.2.1 albedos - compute snow/ice albedos and aggregate . . . . . . . . . . . . . . . . . . . . 13 4.3 Fortran: Module Interface ice atmo - atm-ice interface: stability based flux calculations (Source File: ice atmo.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13 4.3.1 stability - compute coefficients for atm-ice fluxes, stress and Tref . . . . . . . . . . . . 14 4.3.2 ice src flux - compute ice-atm surface fluxes . . . . . . . . . . . . . . . . . . . . . . . . 14 4.4 Fortran: Module Interface ice calendar - calendar routines for managing time (Source File:

ice calendar.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 15 4.4.1 init calendar - initialize calendar variables . . . . . . . . . . . . . . . . . . . . . . . . . 15 4.4.2 calendar - computes date at the end of the time step . . . . . . . . . . . . . . . . . . . 16 4.5 Fortran: Module Interface ice constants - sets physical constants (Source File: ice constants.F) 16 4.5.1 init constants - initialize constants defined at run time . . . . . . . . . . . . . . . . . . 17 4.6 Fortran: Module Interface ice coupling - message passing to and from the coupler (Source File: ice coupling.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 17 4.6.1 init cpl - initializes message passing between ice and coupler . . . . . . . . . . . . . . . 17 4.6.2 from coupler - input from coupler to sea ice model . . . . . . . . . . . . . . . . . . . . 18 4.6.3 to coupler - send data from sea ice model to coupler . . . . . . . . . . . . . . . . . . . 18 4.6.4 exit coupler - exit from coupled/mpi environment . . . . . . . . . . . . . . . . . . . . . 19 4.6.5 mpi coupled - sets mpi communicators and component task ids . . . . . . . . . . . . . 19 4.7 Fortran: Module Interface ice dh (Source File: ice dh.F) . . . . . . . . . . . . . . . . . . . . . 20 4.7.1 dh - computes top and bottom thickness changes . . . . . . . . . . . . . . . . . . . . . 20 4.7.2 freeboard - freeboard flooding adjustment: snow-ice formation . . . . . . . . . . . . . 21 4.7.3 srfsub - computes sea ice and snow thickness changes . . . . . . . . . . . . . . . . . . . 22 4.7.4 srfmelt - melt snow and ice from the top . . . . . . . . . . . . . . . . . . . . . . . . . . 22 4.7.5 botmelt - melt from bottom . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 23 4.7.6 adjust - adjusts temperature profile to changing layer spacing . . . . . . . . . . . . . . 24 4.7.7 real function energ - compute energy of melting per unit volume . . . . . . . . . . . . 24 4.8 Fortran: Module Interface ice diagnostics - diagnostic information output during run (Source File: ice diagnostics.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 25 4.8.1 runtime diags - writes max,min,global sums to standard out . . . . . . . . . . . . . . . 25 4.8.2 init mass diags - computes global combined ice and snow mass sum . . . . . . . . . . 25 4.8.3 init diags - initialize diagnostic output . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 4.8.4 print state - print ice state for specified grid point . . . . . . . . . . . . . . . . . . . . 26 4.9 Fortran: Module Interface ice domain - sets array sizes for local subdomain and parallel info (Source File: ice domain.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 4.10 Fortran: Module Interface ice dyn evp - elastic-viscous-plastic sea ice dynamics model (Source File: ice dyn evp.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 4.10.1 evp - elastic-viscous-plastic dynamics driver . . . . . . . . . . . . . . . . . . . . . . . . 28 4.10.2 init evp - initialize parameters needed for evp dynamics . . . . . . . . . . . . . . . . . 28 4.10.3 evp prep - compute quantities needed for stress tensor and mom eqns . . . . . . . . . 28

4.10.4 stress - computes strain rates and internal stress components . . . . . . . . . . . . . . 29 4.10.5 stepu - surface stresses and integrates mom eqn for u,v . . . . . . . . . . . . . . . . . . 29 4.10.6 evp finish - calculates ice-ocean stress . . . . . . . . . . . . . . . . . . . . . . . . . . . 30 4.10.7 principal stress - computes principal stress for yield curve . . . . . . . . . . . . . . . . 30 4.11 Fortran: Module Interface ice flux - flux variable declarations: from, to coupler and internal (Source File: ice flux.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 30 4.11.1 init flux atm - initialize all atmospheric fluxes sent to coupler . . . . . . . . . . . . . . 31 4.11.2 init flux ocn - initialize ocean fluxes sent to coupler . . . . . . . . . . . . . . . . . . . . 31 4.11.3 merge fluxes - aggregate flux information over ITD . . . . . . . . . . . . . . . . . . . . 31 4.12 Fortran: Module Interface ice grid - spatial grids, masks and boundary conditions (Source File: ice grid.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 32 4.12.1 init grid - horizontal grid initialization . . . . . . . . . . . . . . . . . . . . . . . . . . . 32 4.12.2 popgrid - reads and sets pop displaced pole grid and land mask . . . . . . . . . . . . . 33 4.12.3 columngrid - column grid and mask . . . . . . . . . . . . . . . . . . . . . . . . . . . . 33 4.12.4 rectgrid - regular rectangular grid and mask . . . . . . . . . . . . . . . . . . . . . . . . 34 4.12.5 makemask - makes logical land masks (T,U) and hemispheric masks . . . . . . . . . . 34 4.12.6 Tlatlon - initializes latitude and longitudes on T grid . . . . . . . . . . . . . . . . . . . 34 4.12.7 t2ugrid - transfer from T-cell centers to U-cell centers . . . . . . . . . . . . . . . . . . 35 4.12.8 to ugrid - shift from T-cell to U-cell midpoints . . . . . . . . . . . . . . . . . . . . . . 35 4.12.9 u2tgrid - transfer from U-cell centers to T-cell centers . . . . . . . . . . . . . . . . . . 36 4.12.10 to tgrid - shifts array from U-cell to T-cell midpoints . . . . . . . . . . . . . . . . . . . 36 4.12.11 bound - fills ghost cells with boundary information . . . . . . . . . . . . . . . . . . . . 36 4.12.12 bound sw - fills south and west ghost cells . . . . . . . . . . . . . . . . . . . . . . . . . 37 4.12.13 bound narr ne - fills north and east ghost cells . . . . . . . . . . . . . . . . . . . . . . 37 4.12.14 bound narr - fills north and east ghost cells with boundary info . . . . . . . . . . . . . 37 4.12.15 bound ijn - Periodic/Neumann boundary conditions . . . . . . . . . . . . . . . . . . . 38 4.12.16 bound nij - Periodic/Neumann boundary conditions . . . . . . . . . . . . . . . . . . . 38 4.13 Fortran: Module Interface ice history - ice model history and restart files (Source File:

ice history.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 39 4.13.1 init hist - initialize history files . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 39 4.13.2 ice write hist - write average ice quantities or snapshots . . . . . . . . . . . . . . . . . 39 4.13.3 icecdf - write netCDF history file . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 40 4.13.4 nf stat check - check error code returned from netCDF call . . . . . . . . . . . . . . . 40 4.13.5 integer function lenstr(label) - compute length string . . . . . . . . . . . . . . . . . . . 41 4.13.6 dumpfile - dumps all fields required for restart . . . . . . . . . . . . . . . . . . . . . . 41 4.13.7 restartfile - restarts from a dumpfile . . . . . . . . . . . . . . . . . . . . . . . . . . . . 42 4.14 Fortran: Module Interface ice init - parameter and variable initializations (Source File: ice init.F) 42 4.14.1 input data - namelist variables . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 42 4.14.2 init state - initialize state for itd . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 43 4.14.3 init flux - initialize fluxes exchanged with coupler . . . . . . . . . . . . . . . . . . . . . 43 4.14.4 setup mpi - initialize mpi . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 44 4.15 Fortran: Module Interface ice itd - initialize and redistribute ice in the ITD (Source File:

ice itd.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 44 4.15.1 init itd - initalize area fraction and thickness boundaries for ITD . . . . . . . . . . . . 45 4.15.2 aggregate - aggregate ice state over the grid . . . . . . . . . . . . . . . . . . . . . . . . 45 4.15.3 aggregate pt - aggregate a point over ITD state . . . . . . . . . . . . . . . . . . . . . . 45 4.15.4 to column - define column state variables for given point . . . . . . . . . . . . . . . . . 46 4.15.5 from column - reload state variables from given point . . . . . . . . . . . . . . . . . . 46 4.15.6 check state - require certain fields to be monotone . . . . . . . . . . . . . . . . . . . . 46 4.15.7 distr check - enforce ice area minimum and ice thickness boundaries . . . . . . . . . . 47 4.15.8 normalize state - normalize ice state after small areas removed . . . . . . . . . . . . . 47 4.15.9 rebin ice - rebins thicknesses into defined categories . . . . . . . . . . . . . . . . . . . 48 4.15.10 movedn - moves ice from cat 2 to cat 1 . . . . . . . . . . . . . . . . . . . . . . . . . . 48 4.15.11 moveup - moves ice from cat 1 to cat 2 . . . . . . . . . . . . . . . . . . . . . . . . . . . 49

4.15.12 zerocat - reset category variables to zero when no ice . . . . . . . . . . . . . . . . . . . 50 4.16 Fortran: Module Interface ice itd linear - linear remapping scheme for ITD (Source File:

ice itd linear.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 50 4.16.1 linear itd - ITD scheme that shifts ice among categories . . . . . . . . . . . . . . . . . 51 4.16.2 fit line - fit g(h) with a line using area, volume constraints . . . . . . . . . . . . . . . . 52 4.16.3 shift ice - shift ice across category boundaries . . . . . . . . . . . . . . . . . . . . . . 52 4.17 Fortran: Module Interface ice kinds mod - defines variable precision (Source File: ice kinds mod.F) 53 4.18 Fortran: Module Interface ice mechred - computes mech redistribution and strength for ITD (Source File: ice mechred.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 53 4.18.1 init mechred - initialize constants for ridging . . . . . . . . . . . . . . . . . . . . . . . 54 4.18.2 mechanical redistr - driver for ridging . . . . . . . . . . . . . . . . . . . . . . . . . . . 54 4.18.3 ridge - ridge ice due to convergence or shear deformation . . . . . . . . . . . . . . . . 55 4.18.4 ridging mode - compute W and Wa factors . . . . . . . . . . . . . . . . . . . . . . . . 55 4.18.5 ridge matrices - compute Gamma factors . . . . . . . . . . . . . . . . . . . . . . . . . 56 4.18.6 comp matrices - compute Gamm functions . . . . . . . . . . . . . . . . . . . . . . . . 56 4.18.7 real function roth strength - Rothrock ice strength . . . . . . . . . . . . . . . . . . . . 57 4.19 Fortran: Module Interface ice model size - defines global domain size, category and layer number (Source File: ice model size.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 57 4.20 Fortran: Module Interface ice mpi internal - parameters and common blocks for MPI internal to ice model (Source File: ice mpi internal.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . 58 4.20.1 ice global real minmax - computes global min/max and prints . . . . . . . . . . . . . 58 4.20.2 real function ice global real minval - computes global min . . . . . . . . . . . . . . . . 58 4.20.3 real function ice global real maxval - computes global max . . . . . . . . . . . . . . . 59 4.20.4 real function ice global real sum - sums input array over global grid . . . . . . . . . . 59 4.20.5 ice bcast logical - broadcasts scalar logical to all processors . . . . . . . . . . . . . . . 59 4.20.6 ice bcast char - broadcasts scalar character to all processors . . . . . . . . . . . . . . . 60 4.20.7 ice bcast rscalar - broadcasts real scalar all processors . . . . . . . . . . . . . . . . . . 60 4.20.8 ice bcast iscalar - broadcasts integer scalar all processors . . . . . . . . . . . . . . . . 61 4.20.9 global scatter - scatters global to distributed array, adding ghost cells . . . . . . . . . 61 4.20.10 global gather - gathers distributed array into global array . . . . . . . . . . . . . . . . 61 4.20.11 get sum - computes weighted sum over global grid . . . . . . . . . . . . . . . . . . . . 62 4.20.12 end run - ends run . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 62 4.21 Fortran: Module Interface ice ocean - ocean mixed layer internal to sea ice model (Source File: ice ocean.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 63 4.21.1 init oceanmixed ice - initialize mixed layer forcing data . . . . . . . . . . . . . . . . . 63 4.21.2 time intrplt ocean forcing - time interpolates ocean forcing . . . . . . . . . . . . . . . 64 4.21.3 set oceanmixed ice - set sst and frzmlt . . . . . . . . . . . . . . . . . . . . . . . . . . . 64 4.21.4 compute oceanmixed ice - update ocean state fields . . . . . . . . . . . . . . . . . . . 65 4.21.5 mixed layer(i,j) - computes open ocean fluxes . . . . . . . . . . . . . . . . . . . . . . . 65 4.21.6 ocnheat(i,j, delt, delq) - update ocean fields . . . . . . . . . . . . . . . . . . . . . . . 66 4.22 Fortran: Module Interface ice prescribed - Prescribed Ice (Source File: ice prescribed.F) . . . 66 4.22.1 init prescribed ice - initialize prescribed ice data . . . . . . . . . . . . . . . . . . . . . 67 4.22.2 read prescribed ice - read in two ice concentration fields . . . . . . . . . . . . . . . . . 67 4.22.3 read prescribed ice climate - read two climate ice concentrations . . . . . . . . . . . . 68 4.22.4 set prescribed ice state - set prescribed ice state . . . . . . . . . . . . . . . . . . . . . 68 4.22.5 set prescribed ice flux - Set non-computed fluxes to zero . . . . . . . . . . . . . . . . . 69 4.22.6 exit prescribed ice - close netCDF file for prescribed ice . . . . . . . . . . . . . . . . . 69 4.23 Fortran: Module Interface ice prnpnt - diagnostic grid point info during execution (Source File: ice prnpnt.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 69 4.23.1 intpnt - initializes printout of grid point data . . . . . . . . . . . . . . . . . . . . . . . 70 4.23.2 diags cpl in - grid point printout of input info from coupler . . . . . . . . . . . . . . . 70 4.23.3 diags cpl out - grid point printout of info sent to coupler . . . . . . . . . . . . . . . . . 70 4.24 Fortran: Module Interface ice read write - routines for opening, reading and writing external files (Source File: ice read write.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 71

4.24.1 ice open - opens an unformatted file for reading . . . . . . . . . . . . . . . . . . . . . . 71 4.24.2 ice read - reads an unformatted file . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 72 4.24.3 ice write - writes an unformatted file . . . . . . . . . . . . . . . . . . . . . . . . . . . . 72 4.25 Fortran: Module Interface ice scaling - scale ice (Source File: ice scaling.F) . . . . . . . . . . 72 4.25.1 scale fluxes - scale fluxes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 73 4.25.2 scale hist fluxes - scale history fluxes . . . . . . . . . . . . . . . . . . . . . . . . . . . . 73 4.26 Fortran: Module Interface ice state - primary state variables (Source File: ice state.F) . . . . 74 4.27 Fortran: Module Interface ice therm driver - driver for thermodynamics and itd (Source File:

ice therm driver.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 74 4.27.1 thermo rates - compute thermo growth rates and atm fluxes . . . . . . . . . . . . . . . 75 4.27.2 thermo itd - changes in itd due to thermodynamic growth . . . . . . . . . . . . . . . . 75 4.27.3 init column diags - initialize column diagnostics . . . . . . . . . . . . . . . . . . . . . . 76 4.27.4 init vertical profile - initialize vertical ice profile . . . . . . . . . . . . . . . . . . . . . 76 4.27.5 init frzmlt - initialize ocean-ice heat fluxes, bottom and lateral . . . . . . . . . . . . . 77 4.27.6 lateral growth melt - frazil ice growth and lateral melt . . . . . . . . . . . . . . . . . . 77 4.27.7 reduce area - reduce area when ice melts for special case ncat=1 . . . . . . . . . . . . 78 4.27.8 conservation check - enforce ice property conservation . . . . . . . . . . . . . . . . . . 78 4.28 Fortran: Module Interface ice timers (Source File: ice timers.F) . . . . . . . . . . . . . . . . . 79 4.28.1 ice timer clear(n) - initialize timer n to 0 . . . . . . . . . . . . . . . . . . . . . . . . . 79 4.28.2 ice timer start(n) - begin timing with timer n . . . . . . . . . . . . . . . . . . . . . . . 80 4.28.3 ice timer stop(n) - end (or pause) timing with timer n . . . . . . . . . . . . . . . . . . 80 4.28.4 ice timer print(n) - print timing results of timer n . . . . . . . . . . . . . . . . . . . . 80 4.28.5 timers(t1) - do the work . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 81 4.29 Fortran: Module Interface ice transport - horizontal advection (via mpdata) (Source File:

ice transport.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 81 4.29.1 transport - computes transport equations for one timestep . . . . . . . . . . . . . . . . 82 4.29.2 mpdata(narrays,phi) - advection according to mpdata . . . . . . . . . . . . . . . . . . 82 4.30 Fortran: Module Interface ice tstm - energy conserving sea ice model thermodynamics (Source File: ice tstm.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 83 4.30.1 tstm - calculates surface and internal snow/ice temp . . . . . . . . . . . . . . . . . . . 83 4.30.2 getabc - computes elements of tridiagonal matrix . . . . . . . . . . . . . . . . . . . . . 84 4.30.3 tridag - solves tridiagonal equations . . . . . . . . . . . . . . . . . . . . . . . . . . . . 85 4.30.4 conductiv - calculates T,S dependent conductivity . . . . . . . . . . . . . . . . . . . . 85 4.31 Fortran: Module Interface ice vthermo - main routines for energy-conserving vertical thermodynamics (Source File: ice vthermo.F) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 86 4.31.1 init thermo - setup salinity profile and tmelt for each layer . . . . . . . . . . . . . . . 86 4.31.2 thermo vertical - heat budget over open water and ice . . . . . . . . . . . . . . . . . . 87

5 Making Modifications to Code 87 5.1 Adding Fields to the History File . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 88 5.2 Changing Algorithms . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 88 5.3 Adding Prognostic Fields . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 88 5.4 Modifying Restart Files . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 88

6 Miscellaneous Features 88 6.1 Diagnostic Printouts . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 89 6.2 Water and Energy Budgets . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 89

7 Summary 89

1 Introduction

The Community Climate System Model (CCSM) is a coupled climate model consisting of atmosphere, ocean, land, and sea ice components which exchange fluxes and states through a coupler. This model is making important contributions to knowledge about past, present, and future climates.

The sea ice component of CCSM Version 2 is the Community Sea Ice Model Version 4, or CSIM4. The physics of this component is described in Briegleb et al. (2002). Accessing and running CSIM4 is described in Schramm (2002). This document discusses the CSIM4 source code, its general organization and data structures, a detailed listing of all modules (including subroutines, module reference and input/output arguments), how to add new fields to the history file, and finally suggestions on modifying the source code.

2 Overview of CSIM4 Code

The CSIM4 source code is maintained in the Concurrent Version System (CVS) at NCAR. It can be accessed off the web, or by a CVS checkout (co) command online at NCAR. The source code is written in Fortran 90, and consists of thirty-one files all resident in a single source directory. The main driver file is ’ice.F’, which runs the sea ice model.

Each source code file contains a single module of the same name as the file (excluding the suffix .F), with the exception of the main driver file (ice.F). For example, the file ice scaling.F contains the module ice scaling. Within most modules are various data declarations and subroutines, along with protex commands for automatic documentation.

The modules can be organized as in Table 1 in the approximate order of call in the driver file ice.F. The four modules at the end of the table refer to optional and io routines. The logical structure of the code is: initialization and time stepping loop, which involves receiving forcing data from the coupler, a partial thermodynamic calculation to compute the flux exchange with the atmosphere, sending of the output to the coupler, completion of the thermodynamic calculation, linear remapping, calculation of the ice velocities, advection, mechanical redistribution and albedos. Note that while this logical structure is present in the driver ice.F, the reader must wade through the options of prescribed ice and ocean mixed layer to actually recognize it as these options alter the calling sequence.

This particular order of computations is necessary for coupled model accuracy as well as load balancing. For accuracy in radiant energy absorbed, the albedos used by the atmosphere in calculating the down shortwave should be the same as those used in the surface energy absorption in the sea ice thermodynamics. This requires that the snow/ice albedos be updated in the sea ice model after the thermodynamic calculation with the down shortwave is completed. For load balancing, the atmosphere and sea ice can run in parallel more efficiently if the atmosphere-ice surface exchange is separated from the rest of the sea ice thermodynamics. Hence, the sea ice model computes the atmosphere-ice fluxes as soon as it receives forcing data from the coupler, and returns the output fluxes to the coupler as soon as they are computed.

Because the sea ice model domain is limited globally, further improvements in load balancing arise from limiting the total amount of data exchanged between the sea ice model and the coupler (further explained in the Data Structure’s section).

It should be noted that the coupler requires the fluxes to be in the form of per unit ice area (for it summation over ocean/land/ice fluxes in exchange with the atmosphere). Thus, the atmosphere-ice fluxes computed in the ice model (aggregated over thickness distribution) are further divided by the aggregate ice area (see module ice scaling) before being sent to the coupler.

Table 1: Source Code Modules Module Description

ice.F Main driver

—ice mpi internal.F Sets MPI tasks —ice timers.F Timers for performance

—ice model size.F Defines global domain, category, layer sizes —ice kinds mod.F Definitions of common data types —ice state.F Defines ice state variables —ice domain.F Local domain sizes; parallel info

——ice constants.F Sets physical constants ——ice init.F Parameter and variable initilizations ——ice grid.F Spatial grids, masks and boundary conditions ——ice calendar.F Calendar routines for managing time ——ice flux.F Assigns flux arrays: from, to coupler and internal ——ice itd.F Initilizes and redistributies ice in the itd

——ice therm driver.F Driver for thermodynamics and itd ———ice atmo.F Calculate atmosphere-ice stability based fluxes ———ice vthermo.F Sets up vertical thermodynamics ———ice tstm.F Energy conserving thermodynamics ———ice dh.F Grow/melt snow/ice and adjust temperature profile ———ice itd linear.F Linear remapping scheme for itd

——ice scaling.F Scale fluxes to coupler ——ice coupling.F Message passing to and from coupler

——ice dyn evp.F EVP dynamics ——ice transport.F Advection ——ice mechred.F Mechanical redistribution ——ice albedo.F Snow/Ice albedo

——ice history.F Restart and history files ——ice diagnostics.F Diagnostic printout

—ice prnpnt.F Print data for selected points —ice read write.F Read/write io

—ice ocean.F Slab ocean mixed layer —ice prescribed.F Prescribed ice

2.1 Calling Tree

This section contains the primary calling tree for the coupled ice model. Calls to MPI, netCDF, and share code routines are not included as well as calls to subroutines or functions within the ice model that do not include ice physics (i.e. global scatter, get sum, bound, etc.). Calls to the prescribed ice routines and the ocean mixed layer model within the ice model are shown in parentheses.

ICEMODEL
+-SETUP_MPI-+-MPI_COUPLED
-----------------------
Initialize model
-----------------------
+-INIT_CONSTANTS
+-INPUT_DATA
+-INIT_GRID
| +-POPGRID-+-ICE_OPEN
| | +-ICE_READ
| +-TLATLON
| +-MAKEMASK
+-INIT_CALENDAR
+-INIT_HIST
+-INIT_EVP
+-INIT_FLUX-+-INIT_FLUX_ATM
| +-INIT_FLUX_OCN
+-INIT_ITD
+-INIT_THERMO
+-INIT_MECHRED-+-COMP_MATRICES
+-INIT_STATE-+-AGGREGATE
+-(INIT_PRESCRIBED_ICE)
+-RESTARTFILE-+-AGGREGATE
+-ALBEDOS
+-CALENDAR
+-(INIT_OCEANMIXED_ICE)
+-INIT_CPL-+-CALENDAR
| +-TO_COUPLER-+-DIAGS_CPL_OUT
+-INIT_DIAGS
+-INTPNT
+-ICE_WRITE_HIST+-ICECDF
-----------------------
Begin timestepping loop
-----------------------
+-FROM_COUPLER-+-T2UGRID
| +-DIAGS_CPL_IN
+-(SET_OCEANMIXED_ICE)
+-(READ_PRESCRIBED_ICE_CLIMATE)
+-(READ_PRESCRIBED_ICE)
+-(SET_PRESCRIBED_ICE_STATE)-+-(AGGREGATE)
+-(SET_PRESCRIBED_ICE_FLUX)-+-(INIT_FLUX_ATM)
| +-(INIT_FLUX_OCN)
+-INIT_MASS_DIAGS
+-THERMO_RATES-+-INIT_COLUMN_DIAGS
| +-TO_COLUMN
| +-INIT_FRZMLT
| +-INIT_VERTICAL_PROFILE

| +-THERMO_VERTICAL-+-STABILITY
| | +-ICE_SFC_FLUX
| | +-TSTM
| | +-DH
| | +-MERGE_FLUXES
| +-FROM_COLUMN
+-SCALE_FLUXES
+-TO_COUPLER-+-DIAGS_CPL_OUT
+-(TIME_INTRPLT_OCEAN_FORCING)
+-(COMPUTE_OCEANMIXED_ICE)-+-(MIXED_LAYER)-+-(STABILITY)
| +-(OCNHEAT)
+-THERMO_ITD-+-INIT_FLUX_OCN
| +-TO_COLUMN
| +-LINEAR_ITD-+-AGGREGATE_PT
| | +-PRINT_STATE-+-TO_COLUMN
| | +-FIT_LINE
| | +-SHIFT_ICE
| +-LATERAL_GROWTH_MELT
| +-REDUCE_AREA
| +-REBIN_ICE-+-MOVEUP--ZEROCAT
| | +-MOVEDN--ZEROCAT
| +-AGGREGATE_PT
| +-CONSERVATION_CHECK-+-PRINT_STATE
| +-FROM_COLUMN
| +-CHECK_STATE
+-EVP-+-BOUND_SW--BOUND_IJN
| +-EVP_PREP-+-T2UGRID-+-BOUND
| | | +-TO_UGRID
| | +-TO_UGRID
| +-STRESS
| +-STEPU-+-BOUND_NARR_NE--BOUND_NIJ
| +-EVP_FINISH-+-U2TGRID-+-BOUND
| +-TO_TGRID
+-TRANSPORT-+-BOUND_NARR--BOUND_IJN
| +-MPDATA-+-BOUND_NARR
+-MECHANICAL_REDISTR-+-TO_COLUMN
| +-RIDGE-+-RIDGE_MATRICES-+-COMP_MATRICES
| | +-RIDGING_MODE
| +-ROTH_STRENGTH-+-RIDGING_MODE
| +-FROM_COLUMN
+-DISTR_CHECK-+-TO_COLUMN
| +-MOVEUP
| +-MOVEDN
| +-REBIN_ICE
| +-FROM_COLUMN
| +-NORMALIZE_STATE
+-AGGREGATE
+-SCALE_HIST_FLUXES
+-RUNTIME_DIAGS
+-DUMPFILE-+-ICE_OPEN
| +-ICE_WRITE
-----------------------
End timestepping loop
-----------------------

+-(EXIT_PRESCRIBED_ICE)
+-EXIT_COUPLER

3 Data Structures

Both horizontal and vertical discretization of the sea ice model is presented here, as well as category discretization. Two forms of horizontal discretization are distinguished: a global 2D domain decomposition, and an exclusion of lower latitude regions of no ice in the exchange with the coupler. The ice thickness category discretization can be thought of as a horizontal discretization by ice thickness. The vertical discretization varies with ice thickness category.

3.1 Horizontal

The horizontal computational grid is decomposed into two dimensions for efficiency in parallelization. The global horizontal domain of dimensions imt_{global} × jmt_{global} (for example, the gx1 grid has imt_{global} = 320 longitude points and jmt_{global} = 384 latitude points) is divided into integral NX longitude by NY latitude rectangular subdomains of dimensions (imt_{local} = imt_{global}/NX + 2n_{ghost} + 1) × (jmt_{local} = jmt_{global}/NY + 2n_{ghost} + 1), where imt_{global}/NX, jmt_{global}/NY must be integers (see module ice domain). Each subdomain has a physical portion indexed as [ilo : ihi, jlo : jhi] with n_{ghost} boundary cells outside. Periodic boundary conditions are applied, with boundary routines performing communications between subdomains when running parallel. Global scatter and gather routines distribute information from the global domain to the subdomains and back, respectively (see the “bound” routines in module ice grid).

The thermodynamic calculations involve one grid point at a time (see module ice therm driver) so that a purely thermodynamic model integration is bit-for-bit independent of the domain decompostion (i.e. the exact values of NX, NY ), while the dynamic calculation depends bit-for-bit upon domain boundary conditions, and therefore on the exact values of NX and NY . The sea ice model climate is not sensitive to the precise domain decomposition.

The actual source code uses NP ROC X and NP ROC Y for NX and NY respectively, referring to the number of processors in the x direction and in the y direction (these parameters are set by a pre-compiler; see the CSIM User’s Guide Version 4). The module ice domain defines the local subdomain dimensions and their beginning/ending indices. Module ice init computes and assigns the subdomain processor numbers. The module ice model size assigns the global domain values.

The module ice coupling handles the ’unpacking’ and ’packing’ of the data horizontally after and before exchange with the coupler. This involves excluding latitude bands around the equator that have no sea ice present. Information on the number of latitude bands of data for each hemisphere (i.e. the number of latitude bands of actual hemispheric sea ice but with sufficient equatorwards bands to allow for ice formation along ice edge as well) is included in the data exchange header. As the areas where new ice formation will occur are known to the coupler (based on the freeze/melt potential received from the ocean model), the coupler is able to determine the precise latitude limits. Regions with no ice in the unpacked fields are simply filled with zeros after being received from the coupler.

3.2 Category

The number of ice thickness categories (ncat) is assigned in module ice model size. The state variables which vary with category are found in module ice state. Note that only aggregate quantities (i.e. averaged over the ice thickness distribution) are exchanged with the coupler.

3.3 Vertical

Vertically, sea ice is discretized into L evenly spaced layers, where the number of layers of ice (L) depends on the thickness category, with the thinnest two categories having two equally spaced layers and the thicker three categories having four. The total sum of vertical levels for all categories is specified in module ice model size as ntilay, with the maximum number of levels for any category being nmax. Several state variables are dependent on vertical level, as seen in module ice state.

4 Module Descriptions

In this section, we present a detailed module-by-module listing of the CSIM4 source code. This text was generated using protex, which uses embedded key words in the source code itself. Using the protex commands and structure allows one to maintain and update internal documentation in the source code from which external code documentation can be generated. See Table 2 for the protex keywords embedded in the source code. Each protex keyword and description text is headed by exclamation mark (!), and ends with a colon (:), excepting the beginning and ending keywords. All protex keywords and description lines must lie within the protex beginning and ending keywords. Within a description section, latex is used to interpret the text, and so in particular two backslashes are used as carriage return, and backslash underscore is used for underscore.

Table 2: Protex Keywords Keyword Description !BOP Beginning of protex section !EOP End of protex section !MODULE: Module name follows on same line !DESCRIPTION: Description section in latex !REVISION HISTORY: Gives author and revision information !INTERFACE: Actual fortran module or subroutine statement !USES: Sets off module uses declaration section !IROUTINE: Routine name and one line description !INPUT/OUTPUT PARAMETERS: Input/Output declaration section follows

4.1 Fortran: Module Interface icemodel - main ice model program (Source File:

ice.F)

The NCAR Community Climate System Model Version 2 - Sea Ice (CCSM2-SI) is intended for use by the climate modeling community, and its development has been a true community effort. The list of physics to be included in CCSM2-SI was developed by the CCSM Polar Climate Working Group (PCWG) in a series of meetings during 1997-1999. The specific parameterizations and codes to be implemented were identified and agreed upon at a meeting of ice model developers from the PCWG, held at NCAR in September, 1999.

A brief description of the development of the CCSM2-SI code is as follows:

o The code originated from the LANL CICE model (version of September, 1999). CCSM2-SI retains the following elements from this original code: Elastic-viscous-plastic dynamics (EVP), MPDATA transport scheme, and much of the original code structure.

o Later in autumn of 1999, the code was changed as follows: (1) the MPI parallelization routines were updated; (2) a multi-category ice thickness distribution was added; (3) a new thermodynamic code with explicit treatment of brine pockets was added.

o In late 1999/early 2000, changes were made to the history output.

o During winter-spring 2000, the Active Ice Only (AIO) framework was developed, together with datasets to be used as forcing within this framework. The model was tested within this AIO framework.

o In the fall of 2000, the code was streamlined, checked, standardized, and updated to Fortran 90. Documentation is currently being written.

The development team for the model described above is:

Elizabeth Hunke, LANL Cecilia Bitz, U. WA. Bruce Briegleb, NCAR Tony Craig, NCAR Marika Holland, NCAR Bill Lipscomb, LANL Julie Schramm, NCAR

Numerous others have contributed to this effort also–thanks to all!

INTERFACE:

program icemodel

USES:

use ice_timers
use ice_mpi_internal
use ice_albedo
use ice_vthermo
use ice_mechred
use ice_scaling
use ice_diagnostics
use ice_history
use ice_coupling
use ice_grid
use ice_calendar
use ice_dyn_evp
use ice_itd
use ice_itd_linear
use ice_transport
use ice_therm_driver
use ice_init
use shr_msg_mod,only:shr_msg_chdir,shr_msg_dirio,shr_sys_flush
use ice_prescribed
use ice_ocean
use ice_prnpnt

REVISION HISTORY:

February 2001 - E.Hunke (LANL) provided original
May 2001 - Final form settled (M.Holland, J.Schramm and
                B.Briegleb, NCAR)

4.2 Fortran: Module Interface ice albedo - snow and ice albedo parameterization (Source File: ice albedo.F)

The albedo parameterization

REVISION HISTORY:

authors: Bruce P. Briegleb, NCAR
          Elizabeth C. Hunke, LANL

INTERFACE:

module ice_albedo

USES:

use ice_kinds_mod
use ice_domain

4.2.1 albedos - compute snow/ice albedos and aggregate

INTERFACE:

subroutine albedos

DESCRIPTION:

Compute albedos and aggregate them note: ice albedo is zero if no ice present REVISION HISTORY:

authors: Bruce P. Briegleb, NCAR
          Elizabeth C. Hunke, LANL

USES:

use ice_constants
use ice_grid
use ice_state

INPUT/OUTPUT PARAMETERS:

4.3 Fortran: Module Interface ice atmo - atm-ice interface: stability based flux calculations (Source File: ice atmo.F)

Atmospheric boundary interface (stability based flux calculations) REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

INTERFACE:

module ice_atmo

USES:

use ice_domain
use ice_constants
use ice_flux
use ice_state

4.3.1 stability - compute coefficients for atm-ice fluxes, stress and Tref

INTERFACE:

 subroutine stability( i,j,nc, Tsf, rdn_in,
$ strx ,stry ,Trf, dssqdt, delt, delq)

DESCRIPTION:

Compute coefficients for atm/ice fluxes, stress, and reference temperature. NOTE: (1) all fluxes are positive downward, (2) net heat flux = fswabs + flwup + (1-emissivity)flwdn + fsh + flh, (3) here, tstar = (WT)/U*, and qstar = (WQ)/U*, (4) wind speeds should all be above a minimum speed (eg. 1.0 m/s). ASSUME:

The saturation humidity of air at T(K): qsat(T) (kg/m**3) Code originally based on CSM1

REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j,nc
 real (kind=dbl_kind), intent(in) ::
& Tsf ! surface temperature of ice or ocean
&, rdn_in ! initial value for rdn, dependent on ice/ocean surface
 real (kind=dbl_kind), intent(out) ::
& strx ! x surface stress (N)
&, stry ! y surface stress (N)
&, Trf ! reference height temperature (K)
&, dssqdt ! derivative of ssq wrt Ti (kg/kg/K)
&, delt ! potential T difference (K)
&, delq ! humidity difference (kg/kg)

4.3.2 ice src flux - compute ice-atm surface fluxes

INTERFACE:

 subroutine ice_sfc_flux(i,j,nc, dssqdt, delt, delq,
& flwdabs,flwup, fswabs,fswabsv,fswabsi,
& fsh,flh,dflhdT,dfshdT,dflwdT)

DESCRIPTION:

Compute ice-atm surface fluxes REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_kinds_mod
use ice_albedo

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j,nc
 real (kind=dbl_kind), intent(in) ::
& dssqdt ! derivative of ssq wrt Ti (kg/kg/K)
&, delt ! potential T difference (K)
&, delq ! humidity difference (kg/kg)
 real (kind=dbl_kind), intent(out) ::
& flwdabs ! down long-wave absorbed heat flx (W/m**2)
&, flwup ! emitted long-wave upward heat flux (W/m**2)
&, fswabs ! srfc absrbd short-wave heat flux (W/m**2)
&, fswabsv ! fswabs in vis (wvlngth < 700nm) (W/m**2)
&, fswabsi ! fswabs in nir (wvlngth > 700nm) (W/m**2)
&, fsh ! sensible heat flux (W/m**2)
&, flh ! latent heat flux (W/m**2)
&, dflhdT ! d(flh)/d(T) (W/m**2/K)
&, dfshdT ! d(fsh)/d(T) (W/m**2/K)
&, dflwdT ! d(flwup)/d(T) (W/m**2/K)

4.4 Fortran: Module Interface ice calendar - calendar routines for managing time (Source File: ice calendar.F)

Calendar routines for managing time REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Tony Craig, NCAR

INTERFACE:

module ice_calendar

USES:

use ice_constants

4.4.1 init calendar - initialize calendar variables

INTERFACE:

subroutine init_calendar

DESCRIPTION:

Initialize calendar variables REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

4.4.2 calendar - computes date at the end of the time step

INTERFACE:

subroutine calendar(ttime)

DESCRIPTION:

Determine the date at the end of the time step REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& ttime ! time variable

4.5 Fortran: Module Interface ice constants - sets physical constants (Source File: ice constants.F)

This module defines a variety of physical and numerical constants used throughout the ice model Code originally based on constants.F in POP REVISION HISTORY:

author Elizabeth C. Hunke, LANL

INTERFACE:

module ice_constants

USES:

#ifdef coupled
      use shr_const_mod
#endif
      use ice_kinds_mod
      use ice_domain

4.5.1 init constants - initialize constants defined at run time

INTERFACE:

subroutine init_constants

DESCRIPTION:

Initializes constants that are best defined at run time (e.g. pi) REVISION HISTORY:

author Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

4.6 Fortran: Module Interface ice coupling - message passing to and from the coupler (Source File: ice coupling.F)

Message passing to and from the coupler REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

INTERFACE:

module ice_coupling

USES:

use ice_calendar
use ice_model_size
use ice_prescribed
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

4.6.1 init cpl - initializes message passing between ice and coupler

INTERFACE:

subroutine init_cpl

DESCRIPTION:

Initializes message passing between ice and coupler REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_domain
use ice_constants
use ice_mpi_internal
use ice_grid
use ice_calendar
use ice_history, only : runtype

INPUT/OUTPUT PARAMETERS:

4.6.2 from coupler - input from coupler to sea ice model

INTERFACE:

subroutine from_coupler

DESCRIPTION:

Reads input data from coupler to sea ice model REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_domain
use ice_constants
use ice_flux
use ice_timers
use ice_mpi_internal
use ice_diagnostics
use ice_grid
use ice_calendar
use ice_state
use ice_prnpnt

INPUT/OUTPUT PARAMETERS:

4.6.3 to coupler - send data from sea ice model to coupler

INTERFACE:

subroutine to_coupler

DESCRIPTION:

Sea ice model to coupler REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_model_size
use ice_domain
use ice_constants
use ice_flux
use ice_timers
use ice_mpi_internal
use ice_albedo
use ice_diagnostics
use ice_grid
use ice_calendar
use ice_state
use ice_history, only : sabs
use ice_prnpnt
use ice_prescribed
use ice_ocean

INPUT/OUTPUT PARAMETERS:

4.6.4 exit coupler - exit from coupled/mpi environment

INTERFACE:

subroutine exit_coupler

DESCRIPTION:

Exit from coupled/MPI environment

REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_kinds_mod
use ice_model_size
use ice_domain

INPUT/OUTPUT PARAMETERS:

4.6.5 mpi coupled - sets mpi communicators and component task ids

INTERFACE:

 subroutine mpi_coupled (in_model_name,
& cpl_task, model_task, model_comm)

DESCRIPTION:

This routine queries all the components of the full coupled system and sets up proper communicators and task ids for each component of the coupled system

This routine should be called after mpi-init, but before setting up any internal mpi setups (since these will require the internal communicators returned by this routine) Code originally based on POP routine

REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

include "mpif.h" ! MPI library definitions

INPUT/OUTPUT PARAMETERS:

 character (3), intent(in) :: in_model_name
                   ! 3-letter identifier (atm, lnd, ocn, ice, cpl)
                   ! for the model calling this routine
 integer, intent(out) ::
& cpl_task ! master task of coupler
&, model_task ! master task of model (in MPI_COMM_WORLD)
&, model_comm ! communicator for internal model comms

4.7 Fortran: Module Interface ice dh (Source File: ice dh.F)

Energy-conserving sea ice model Routines to grow/melt ice and adjust temperature profile See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669-15,677.

See Bitz, C.M., M.M. Holland, M. Eby, and A.J. Weaver, 2001: Simulating the ice-thickness distribution in a coupled climate model, J. Geophys. Res., 106, 2441-2464. REVISION HISTORY:

author: C. M. Bitz, UW

INTERFACE:

module ice_dh

USES:

use ice_kinds_mod
use ice_constants
use ice_itd

4.7.1 dh - computes top and bottom thickness changes

INTERFACE:

 subroutine dh( dtsub, sal1d, tiz
$ , tbot, hi, hs, fbot
$ , fnet, condb, flh, ni
$ , dhib, dhit, dhs, subi
$ , subs, dhif, dhsf, qi
$ , focn, i,j )

DESCRIPTION:

Computes the thickness changes at the top and bottom and adjusts layer energy of melt; does not allow h less than 0.

Focn= actual flux of heat from the ocean layer under sea ice (equal to fbot unless all the ice melts away); compensates for rare case of melting entire slab through

REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_state
use ice_diagnostics
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& dtsub ! timestep
&, sal1d (nmax+1) ! ice salinity (ppt)
&, tiz (0:nmax) ! snow/ice internal temp (C)
&, Tbot ! ice bottom in (C)
&, hi ! initial ice thickness (m)
&, hs ! initial snow thickness (m)
&, fbot ! flx from ocean, potent. (W/m**2)
&, fnet ! net flx at top srf incl. cond. flx (W/m**2)
&, condb ! cond. flx at bot. (W/m**2)
&, flh ! latent heat flx (w/m**2)

 integer (kind=int_kind), intent(in) ::
& ni ! number of layers
&, i,j ! grid location for debugging

 ! thickness changes from grow/melt (default) or sublimate/flooding
 real (kind=dbl_kind), intent(out) ::
& dhib ! ice bot, dhib<0 if melt (m)
&, dhit ! ice top, dhit<=0 (m)
&, dhs ! snow top, dhit<=0 (m)
&, subi ! ice top, subi<0 if sublimating (m)
&, subs ! snow, subs<0 if sublimating (m)
&, dhif ! ice top from flooding, dhif>0 (m)
&, dhsf ! snow from flooding, dhsf<0 (m)
&, qi(nmax) ! energy of melt of ice per unit vol. (J/m**3)
&, focn ! actual flx of heat used from ocn (w/m**2)

4.7.2 freeboard - freeboard flooding adjustment: snow-ice formation

INTERFACE:

subroutine freeboard(hs,hi,dhs,qs,dhsf,dhif,qiflood)

DESCRIPTION:

Freeboard adjustment due to flooding ... snow-ice formation

REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& hs ! initial snow thickness (m)
&, hi ! initial ice thickness (m)
&, dhs ! snow top, dhit<=0 (m)
&, qs ! energy of melt of snow per unit vol. (J/m**3)
 real (kind=dbl_kind), intent(out) ::
& dhsf ! snow from flooding, dhsf<0 (m)
&, dhif ! ice top from flooding, dhif>0 (m)
&, qiflood ! energy of melt of flooded ice (W/m**2)

4.7.3 srfsub - computes sea ice and snow thickness changes

INTERFACE:

 subroutine srfsub( qi, qs, delti, delts, ni,
$ subi, subs, etop, enet )

DESCRIPTION:

Compute the sea ice and snow thickness changes from sublimation/condensation REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& qi (1:nmax), qs ! energy of melt of ice/snow per vol (J/m**3)
&, delti(nmax), delts ! thickness of ice/snow layer (m)
 integer (kind=int_kind), intent(in) :: ni ! number of layers
 real (kind=dbl_kind), intent(out) ::
& subi, subs ! subl/cond. amount for ice/snow (m)
 real (kind=dbl_kind), intent(inout) ::
& etop ! energy avail to sub/cond ice/snow (J/m**2)
&, enet ! energy needed to melt all ice/snow (J/m**2)

4.7.4 srfmelt - melt snow and ice from the top

INTERFACE:

 subroutine srfmelt( qi, qs, delti, delts, ni,
$ dhit, dhs, etop )

DESCRIPTION:

Melt ice/snow from the top srf REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& qi (1:nmax), qs ! energy of melt of ice/snow per vol (J/m**3)
&, delti(nmax), delts ! thickness of ice/snow layer (m)
 integer (kind=int_kind), intent(in) :: ni ! number of layers
 real (kind=dbl_kind), intent(out) ::
& dhit ! ice thickness change (m)
&, dhs ! snow thickness change (m)
 real (kind=dbl_kind), intent(inout) ::
& etop ! energy avail to melt ice and snow (J/m**2)

4.7.5 botmelt - melt from bottom

INTERFACE:

 subroutine botmelt( qi, qs, delti, delts, ni,
$ dhib, dhs, ebot )

DESCRIPTION: Melt from bottom REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& qi (1:nmax), qs ! energy of melt of ice/snow per vol (J/m**3)
&, delti(nmax), delts ! thickness of ice/snow layer (m)
 integer (kind=int_kind), intent(in) :: ni ! number of layers
 real (kind=dbl_kind), intent(out) :: dhib ! ice thickness change (m)
 real (kind=dbl_kind), intent(inout) ::
& dhs ! snow thickness change (m)
&, ebot ! energy avail to melt ice and snow (J/m**2)

4.7.6 adjust - adjusts temperature profile to changing layer spacing

INTERFACE:

subroutine adjust(hi0,dhib,dhit,dhif,dhsf,qiflood,qigrow,ni,qi_tw)

DESCRIPTION:

Adjusts temperature profile to account for changing the layer spacing due to growth/melt (incl. subl/cond, flooding). At start the energy of melting was computed after updating tiz from the heat equation. hi is the thickness prior to changes from dhib and dhit; hi tw is the thickness after making these changes; dhib is less than 0 if there is melt at the bottom; dhit is less than 0 if there is melt at the top; generally tw is a suffix to label the adjusted variables. REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& hi0 ! initial ice thickness (m)
&, dhib ! ice bot, dhib<0 if melt (m)
&, dhit ! ice top, dhit<=0 (m)
&, dhif ! ice top from flooding, dhif>0 (m)
&, dhsf ! snow from flooding, dhsf<0 (m)
&, qiflood ! qi for flooded ice (J/m**3)
&, qigrow ! qi for ice growing on bot (J/m**3)
 integer (kind=int_kind), intent(in) :: ni
 real (kind=dbl_kind), intent(inout) ::
& qi_tw(nmax) ! energy of melt of ice per unit vol. (J/m**3)

4.7.7 real function energ - compute energy of melting per unit volume

INTERFACE:

real function energ(Tmp ,sal)

DESCRIPTION:

Compute the energy of melting per unit volume (J/m**3) relative to melting (negative quantity) REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& Tmp ! midpt temperature of ice layer (C)
&, sal ! midpt salinity of ice layer (ppt)

4.8 Fortran: Module Interface ice diagnostics - diagnostic information output during run (Source File: ice diagnostics.F)

Diagnostic information output during run REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Bruce P. Briegleb, NCAR

INTERFACE:

module ice_diagnostics

USES:

use ice_domain
use ice_constants

4.8.1 runtime diags - writes max,min,global sums to standard out

INTERFACE:

subroutine runtime_diags

DESCRIPTION:

Writes diagnostic info (max, min, global sums, etc) to standard out REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Bruce P. Briegleb, NCAR
         Cecilia M. Bitz, UW

USES:

use ice_model_size
use ice_flux
use ice_albedo
use ice_mpi_internal
use ice_history
use ice_grid
use ice_calendar
use ice_state
use ice_dyn_evp
use shr_sys_mod, only : shr_sys_flush

INPUT/OUTPUT PARAMETERS:

4.8.2 init mass diags - computes global combined ice and snow mass sum

INTERFACE:

subroutine init_mass_diags

DESCRIPTION:

Computes global combined ice and snow mass sum REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_mpi_internal
use ice_grid
use ice_state

INPUT/OUTPUT PARAMETERS:

4.8.3 init diags - initialize diagnostic output

INTERFACE:

subroutine init_diags

DESCRIPTION:

Initialize diagnostic output REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

4.8.4 print state - print ice state for specified grid point

INTERFACE:

subroutine print_state(plabel,i,j)

DESCRIPTION:

This routine is useful for debugging call to it should be inserted in the form (after thermo, for example) do j=jlo,jhi -do i=ilo,ihi —call to column(i,j) —plabel = ’post thermo’ —if (istep1.ge.check step.and.i.eq.ip.and.j.eq.jp ——.and.my task.eq.mtask) —call print state(plabel,i,j) -enddo enddo

’use ice diagnostics’ may need to be inserted also, and ’use ice calendar’ if it is not already being used REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_model_size
use ice_kinds_mod
use ice_calendar
use ice_state
use ice_grid
use ice_itd
use ice_flux

INPUT/OUTPUT PARAMETERS:

character (len=20), intent(in) :: plabel
integer (kind=int_kind), intent(in) :: i,j

4.9 Fortran: Module Interface ice domain - sets array sizes for local subdomain and parallel info (Source File: ice domain.F)

Sets array sizes for local subdomain and related parallel processing info. Code originally based on domain.F in POP REVISION HISTORY:

author Elizabeth C. Hunke, LANL

INTERFACE:

module ice_domain

USES:

use ice_kinds_mod
use ice_model_size

4.10 Fortran: Module Interface ice dyn evp - elastic-viscous-plastic sea ice dynamics model (Source File: ice dyn evp.F)

Elastic-viscous-plastic sea ice dynamics model Computes ice velocity See E. C. Hunke and J. K. Dukowicz. An elastic-viscous-plastic model for sea ice dynamics. 1997, J. Phys. Oceanogr., Vol 27, 1849–1867. REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

INTERFACE:

module ice_dyn_evp

USES:

use ice_kinds_mod
use ice_domain
use ice_grid
use ice_constants

4.10.1 evp - elastic-viscous-plastic dynamics driver

INTERFACE:

subroutine evp(kstrngth)

DESCRIPTION:

Elastic-viscous-plastic dynamics driver REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

use ice_timers

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& kstrngth

4.10.2 init evp - initialize parameters needed for evp dynamics

INTERFACE:

subroutine init_evp

DESCRIPTION:

Initialize parameters and variables needed for the evp dynamics REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

use ice_calendar

INPUT/OUTPUT PARAMETERS:

4.10.3 evp prep - compute quantities needed for stress tensor and mom eqns

INTERFACE:

subroutine evp_prep(kstrngth)

DESCRIPTION:

Computes quantities needed in the stress tensor (sigma) and momentum (u) equations, but which do not change during the thermodynamics/transport time step:

–wind stress shift to U grid, –ice mass and ice extent masks, –pressure (strength), and part of the forcing stresses initializes ice velocity for new points to ocean sfc current

REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

use ice_flux
use ice_calendar
use ice_state

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& kstrngth

4.10.4 stress - computes strain rates and internal stress components

INTERFACE:

subroutine stress(ksub)

DESCRIPTION:

Computes the rates of strain and internal stress components for each of the four corners on each T-grid cell REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: ksub ! subcycling step

4.10.5 stepu - surface stresses and integrates mom eqn for u,v

INTERFACE:

subroutine stepu

DESCRIPTION:

Calculation of the surface stresses Integration of the momentum equation to find velocity (u,v) REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

use ice_flux

INPUT/OUTPUT PARAMETERS:

4.10.6 evp finish - calculates ice-ocean stress

INTERFACE:

subroutine evp_finish

DESCRIPTION:

Calculation of the ice-ocean stress ...the sign will be reversed later... REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

use ice_flux

INPUT/OUTPUT PARAMETERS:

4.10.7 principal stress - computes principal stress for yield curve

INTERFACE:

subroutine principal_stress

DESCRIPTION:

Computes principal stresses for comparison with the theoretical yield curve; northeast values REVISION HISTORY:

author: Elizabeth C. Hunke
        Fluid Dynamics Group, Los Alamos National Laboratory

USES:

INPUT/OUTPUT PARAMETERS:

4.11 Fortran: Module Interface ice flux - flux variable declarations: from, to coupler and internal (Source File: ice flux.F)

Flux variable declarations; these include fields sent from the coupler (”in”), sent to the coupler (”out”), and used internally (”internal”) REVISION HISTORY:

author Elizabeth C. Hunke, LANL

INTERFACE:

module ice_flux

USES:

use ice_kinds_mod
use ice_domain
use ice_constants

4.11.1 init flux atm - initialize all atmospheric fluxes sent to coupler

INTERFACE:

subroutine init_flux_atm(i,j)

DESCRIPTION:

Initialize all fluxes sent to coupler for use by the atm model and a few state quantities REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

integer i,j

4.11.2 init flux ocn - initialize ocean fluxes sent to coupler

INTERFACE:

subroutine init_flux_ocn(i,j)

DESCRIPTION:

Initialize fluxes sent to coupler for use by the ocean model REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

integer i,j

4.11.3 merge fluxes - aggregate flux information over ITD

INTERFACE:

 subroutine merge_fluxes(i,j,nc,frshn,evapn,
& fshn,flhn,flwupn,swbot,Focn,Trefn,strxn,stryn)

DESCRIPTION:

Aggregates flux information from all ice thickness categories REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_state

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j,nc
 real (kind=dbl_kind), intent(in) ::
& frshn ! fresh water flux to ocean (kg/m2/s)
&, evapn ! evaporation (kg/m2/s)
&, fshn ! sensible heat flx (W/m**2)
&, flhn ! latent heat flx (W/m**2)
&, flwupn ! upwd lw emitted heat flx (W/m**2)
&, swbot ! sw radiation through ice bot (W/m**2)
&, Focn ! actual ocn/ice heat flx (W/m**2)
&, Trefn ! air tmp rfrnc level (K)
&, strxn ! air/ice zonal strss, (N/m**2)
&, stryn ! air/ice merdnl strss, (N/m**2)

4.12 Fortran: Module Interface ice grid - spatial grids, masks and boundary conditions (Source File: ice grid.F)

Spatial grids, masks, and boundary conditions

REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         Tony Craig, NCAR

INTERFACE:

module ice_grid

USES:

use ice_kinds_mod
use ice_constants
use ice_domain

4.12.1 init grid - horizontal grid initialization

INTERFACE:

subroutine init_grid(oceanmixed_ice)

DESCRIPTION:

Horizontal grid initialization:

HTN,E = cell widths on N,E sides of T cell; ULAT,LONG = true latitude,longitude of U points; DX,YT,U = x,y spacing centered at T,U points.

REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_mpi_internal
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.12.2 popgrid - reads and sets pop displaced pole grid and land mask

INTERFACE:

subroutine popgrid(oceanmixed_ice)

DESCRIPTION:

POP displaced pole grid and land mask. Grid record number, field and units are: (1) ULAT (radians) (2) ULON (radians) (3) HTN (cm) (4) HTE (cm) (5) HUS (cm) (6) HUW (cm) (7) ANGLE (radians).

Land mask record number and field is (1) KMT. REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_read_write

INPUT/OUTPUT PARAMETERS:

4.12.3 columngrid - column grid and mask

INTERFACE:

subroutine columngrid

DESCRIPTION:

Column grid and mask REVISION HISTORY:

author: C. M. Bitz UW, (based on rectgrid by Hunke)

USES:

use ice_model_size
use ice_mpi_internal
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.12.4 rectgrid - regular rectangular grid and mask

INTERFACE:

subroutine rectgrid

DESCRIPTION:

Regular rectangular grid and mask REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

use ice_model_size
use ice_mpi_internal

INPUT/OUTPUT PARAMETERS:

4.12.5 makemask - makes logical land masks (T,U) and hemispheric masks

INTERFACE:

subroutine makemask

DESCRIPTION:

Sets the boundary values for the T cell land mask (hm) and makes the logical land masks for T and U cells (tmask, umask). Also creates hemisphere masks (mask-n northern, mask-s southern) REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

4.12.6 Tlatlon - initializes latitude and longitudes on T grid

INTERFACE:

subroutine Tlatlon

DESCRIPTION:

Initializes latitude and longitude on T grid REVISION HISTORY:

author: Elizabeth C. Hunke, LANL; code originally based on POP grid
generation routine

USES:

use ice_model_size
use ice_mpi_internal
 use ice_read_write ! if reading ULAT, ULON directly from file

INPUT/OUTPUT PARAMETERS:

4.12.7 t2ugrid - transfer from T-cell centers to U-cell centers

INTERFACE:

subroutine t2ugrid(work)

DESCRIPTION:

Transfer from T-cell centers to U-cell centers. Writes work into another array that has ghost cells REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind) :: work (ilo:ihi,jlo:jhi)

4.12.8 to ugrid - shift from T-cell to U-cell midpoints

INTERFACE:

subroutine to_ugrid(work1,work2)

DESCRIPTION:

Shifts quantities from the T-cell midpoint (work1) to the U-cell midpoint (work2) REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind) :: work1(imt_local,jmt_local)
&, work2(ilo:ihi,jlo:jhi)

4.12.9 u2tgrid - transfer from U-cell centers to T-cell centers

INTERFACE:

subroutine u2tgrid(work)

DESCRIPTION:

Transfer from U-cell centers to T-cell centers. Writes work into another array that has ghost cells REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind) :: work (ilo:ihi,jlo:jhi)

4.12.10 to tgrid - shifts array from U-cell to T-cell midpoints

INTERFACE:

subroutine to_tgrid(work1,work2)

DESCRIPTION:

Shifts quantities from the U-cell midpoint (work1) to the T-cell midpoint (work2) REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind) :: work1(imt_local,jmt_local)
&, work2(ilo:ihi,jlo:jhi)

4.12.11 bound - fills ghost cells with boundary information

INTERFACE:

subroutine bound(work1)

DESCRIPTION:

Fills ghost cells with boundary information REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind) :: work1(1)

4.12.12 bound sw - fills south and west ghost cells

INTERFACE:

subroutine bound_sw(work1)

DESCRIPTION:

Fills south and west ghost cells with boundary information REVISION HISTORY:

author: Tony Craig, NCAR

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind) :: work1(1)

4.12.13 bound narr ne - fills north and east ghost cells

INTERFACE:

subroutine bound_narr_ne(narrays,work1)

DESCRIPTION:

Fills north and east ghost cells with boundary information. NOTE: work1 array has form (number-arrays,i-index,j-index) for evp dynamics performance REVISION HISTORY:

authors: Tony Craig, NCAR
         Elizabeth Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind) :: narrays
real (kind=dbl_kind) :: work1(1)

4.12.14 bound narr - fills north and east ghost cells with boundary info

INTERFACE:

subroutine bound_narr(narrays,work1)

DESCRIPTION:

Fills north and east ghost cells with boundary information; narr arrays at once (for performance) REVISION HISTORY:

authors: Tony Craig, NCAR
         Elizabeth Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind) :: narrays
real (kind=dbl_kind) :: work1(1)

4.12.15 bound ijn - Periodic/Neumann boundary conditions

INTERFACE:

subroutine bound_ijn(nd,work1,north,south,east,west)

DESCRIPTION:

Periodic/Neumann conditions for global domain boundaries. Assumptions: a *single* row of ghost cells (num-ghost-cells=1); work1 array has form (i-index,j-index,number-arrays) REVISION HISTORY:

authors: Tony Craig, NCAR
         Elizabeth Hunke, LANL

USES:

use ice_timers
use ice_mpi_internal

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind) :: nd
real (kind=dbl_kind) :: work1(imt_local,jmt_local,nd)
logical north,south,east,west

4.12.16 bound nij - Periodic/Neumann boundary conditions

INTERFACE:

subroutine bound_nij(nd,work1,north,south,east,west)

DESCRIPTION:

Periodic/Neumann conditions for global domain boundaries. Assumptions: a *single* row of ghost cells (num-ghost-cells=1); work1 array has form (number-arrays,i-index,j-index) REVISION HISTORY:

author: Tony Craig, NCAR

USES:

use ice_timers
use ice_mpi_internal

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind) :: nd
real (kind=dbl_kind) :: work1(nd,imt_local,jmt_local)
logical north,south,east,west

4.13 Fortran: Module Interface ice history - ice model history and restart files (Source File: ice history.F)

Output files: netCDF data, Fortran unformatted dumps REVISION HISTORY:

authors Tony Craig, NCAR
        Elizabeth C. Hunke, LANL
        C.M. Bitz, UW
        Bruce P. Briegleb, NCAR

INTERFACE:

module ice_history

USES:

use ice_kinds_mod
use ice_domain
use ice_read_write

4.13.1 init hist - initialize history files

INTERFACE:

subroutine init_hist

DESCRIPTION:

Initialize history files REVISION HISTORY:

authors Tony Craig, NCAR
        Elizabeth C. Hunke, LANL
        C.M. Bitz, UW
        Bruce P. Briegleb, NCAR

USES:

use ice_constants
use ice_calendar
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.13.2 ice write hist - write average ice quantities or snapshots

INTERFACE:

subroutine ice_write_hist

DESCRIPTION:

write average ice quantities or snapshots REVISION HISTORY:

author: E.C.Hunke, LANL

USES:

use ice_flux
use ice_albedo
use ice_mechred
use ice_grid
use ice_calendar
use ice_state
use ice_dyn_evp
use ice_constants

INPUT/OUTPUT PARAMETERS:

4.13.3 icecdf - write netCDF history file

INTERFACE:

subroutine icecdf

DESCRIPTION:

write netCDF history file REVISION HISTORY:

authors: E.C.Hunke, LANL
           Bruce P. Briegleb, NCAR

USES:

use ice_model_size
use ice_constants
use ice_mpi_internal
use ice_grid
use ice_calendar
use ice_itd, only : c_hi_range
use shr_file_mod

INPUT/OUTPUT PARAMETERS:

4.13.4 nf stat check - check error code returned from netCDF call

INTERFACE:

subroutine nf_stat_check (status,msg)

DESCRIPTION:

Check error code returned from netCDF calls If bad, abort REVISION HISTORY:

author: ?

USES:

use shr_sys_mod, only : shr_sys_abort
include "netcdf.inc"

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: status
character (len = *), intent(in) :: msg

4.13.5 integer function lenstr(label) - compute length string

INTERFACE:

integer function lenstr(label)

DESCRIPTION:

Check error code returned from netCDF calls. If bad, abort REVISION HISTORY:

author: ?

INPUT/OUTPUT PARAMETERS:

character*(*) label

4.13.6 dumpfile - dumps all fields required for restart

INTERFACE:

subroutine dumpfile

DESCRIPTION:

Dumps all values needed for a restart REVISION HISTORY:

author Elizabeth C. Hunke, LANL

USES:

use ice_model_size
use ice_flux
use ice_grid
use ice_calendar
use ice_state
use ice_dyn_evp
use shr_file_mod
use ice_ocean

INPUT/OUTPUT PARAMETERS:

4.13.7 restartfile - restarts from a dumpfile

INTERFACE:

subroutine restartfile

DESCRIPTION:

Restarts from a dump REVISION HISTORY:

author Elizabeth C. Hunke, LANL

USES:

use ice_model_size
use ice_flux
use ice_mpi_internal
use ice_grid
use ice_calendar
use ice_state
use ice_dyn_evp
use ice_itd
use ice_ocean

INPUT/OUTPUT PARAMETERS:

4.14 Fortran: Module Interface ice init - parameter and variable initializations (Source File: ice init.F)

parameter and variable initializations REVISION HISTORY:

authors Elizabeth C. Hunke, LANL
        C. M. Bitz

INTERFACE:

module ice_init

USES:

use ice_domain

4.14.1 input data - namelist variables

INTERFACE:

subroutine input_data

DESCRIPTION:

Namelist variables, set to default values; may be altered at run time REVISION HISTORY:

author Elizabeth C. Hunke, LANL

USES:

use ice_mechred
use ice_diagnostics
use ice_history
use ice_calendar
use ice_dyn_evp
use ice_itd
use ice_transport
use ice_prescribed
use ice_ocean
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.14.2 init state - initialize state for itd

INTERFACE:

subroutine init_state

DESCRIPTION:

Initialize state for the itd model REVISION HISTORY:

author C. M. Bitz

USES:

use ice_model_size
use ice_constants
use ice_flux
use ice_vthermo
use ice_grid
use ice_state
use ice_itd
use ice_dh

INPUT/OUTPUT PARAMETERS:

4.14.3 init flux - initialize fluxes exchanged with coupler

INTERFACE:

subroutine init_flux

DESCRIPTION:

Initialize all fluxes exchanged with flux coupler and some data derived fields REVISION HISTORY:

author Elizabeth C. Hunke, LANL

USES:

use ice_constants
use ice_flux

INPUT/OUTPUT PARAMETERS:

4.14.4 setup mpi - initialize mpi

INTERFACE:

subroutine setup_mpi

DESCRIPTION:

This routine initializes mpi for either internal parallel processing or for message passing with the coupler REVISION HISTORY:

author Elizabeth C. Hunke, LANL
code originally based on POP routine

USES:

use ice_mpi_internal
use ice_coupling
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.15 Fortran: Module Interface ice itd - initialize and redistribute ice in the ITD (Source File: ice itd.F)

Routines to initialize the ice thickness distribution and utilities to redistribute ice among categories. These routines are not specific to a particular numerical implementation.

See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669–15,677.

See Bitz, C.M., M.M. Holland, A.J. Weaver, M. Eby, 2001: Simulating the ice-thickness distribution in a climate model, J. Geophys. Res., 106, 2441–2464.

REVISION HISTORY:

author: C. M. Bitz, UW
code heavily modified by Elizabeth C. Hunke, LANL

INTERFACE:

module ice_itd

USES:

use ice_kinds_mod
use ice_model_size
use ice_constants
use ice_state

4.15.1 init itd - initalize area fraction and thickness boundaries for ITD

INTERFACE:

subroutine init_itd

DESCRIPTION:

Initialize area fraction and thickness boundaries for the itd model REVISION HISTORY:

authors: William H. Lipscomb, LANL
         Elizabeth C. Hunke LANL and C. M. Bitz UW

USES:

use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.15.2 aggregate - aggregate ice state over the grid

INTERFACE:

subroutine aggregate

DESCRIPTION:

Aggregate ice state over the grid REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_domain
use ice_flux
use ice_grid

INPUT/OUTPUT PARAMETERS:

4.15.3 aggregate pt - aggregate a point over ITD state

INTERFACE:

subroutine aggregate_pt(i,j)

DESCRIPTION:

Aggregate ice thickness distribution state REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_flux

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: i, j

4.15.4 to column - define column state variables for given point

INTERFACE:

subroutine to_column(i,j)

DESCRIPTION:

Define column state variables for given point (i,j) REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         and C. M. Bitz, UW

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: i,j

4.15.5 from column - reload state variables from given point

INTERFACE:

subroutine from_column(i,j)

DESCRIPTION:

Reload state variables for given point (i,j) from column variables REVISION HISTORY:

authors: Elizabeth C. Hunke, LANL
         and C. M. Bitz, UW

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: i,j

4.15.6 check state - require certain fields to be monotone

INTERFACE:

subroutine check_state(i,j)

DESCRIPTION:

Insist that certain fields are monotone. Should not be necessary if all is well, but best to keep going. Model will not conserve energy and water if fields are zeroed here. REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_flux

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind) :: i,j

4.15.7 distr check - enforce ice area minimum and ice thickness boundaries

INTERFACE:

subroutine distr_check

DESCRIPTION:

Force ice thickness distribution to maintain two rules (1) the fractional area cannot be less than some limiting value (2) each categories thickness lies within the max and min thickness range for that category REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_flux
use ice_grid

INPUT/OUTPUT PARAMETERS:

4.15.8 normalize state - normalize ice state after small areas removed

INTERFACE:

subroutine normalize_state(dvicen,dvices,dvsnon,dvsnos)

DESCRIPTION:

Normalize the state variables for the ice thickness distribution to conserve volume after removing small areas REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_model_size
use ice_mpi_internal
use ice_grid
use ice_calendar

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& dvicen(1), dvsnon(1) ! total nuked ice/snow volumes north
&, dvices(1), dvsnos(1) ! total nuked ice/snow volumes south

4.15.9 rebin ice - rebins thicknesses into defined categories

INTERFACE:

subroutine rebin_ice(i,j)

DESCRIPTION:

Rebins thicknesses into defined categories REVISION HISTORY:

author: C. M. Bitz, UW

USES:

use ice_flux

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& i,j

4.15.10 movedn - moves ice from cat 2 to cat 1

INTERFACE:

 subroutine movedn( Tf0
$ , ai1, vi1, vs1, ei1, Tsf1
$ , hi1, hs1
& , h1min, nn1
$ , ai2, vi2, vs2, ei2, Tsf2
$ , hi2, hs2
& , h2min, nn2 )

DESCRIPTION:

Moves ice from cat 2 to cat 1.

It is possible that the final thickness will be below the boundary of cat 1 if the ice has melted a lot, in which case it will be moved down again by a subsequent call REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& Tf0 ! freezing temperature of ocean
&, h1min, h2min ! minimum thickness range of cat 1, 2 (m)
 integer (kind=int_kind), intent(in) ::
& nn1, nn2 ! number of layers in cat 1, 2

 real (kind=dbl_kind), intent(inout) ::
& ai1, ai2 ! fraction of ice
&, vi1, vi2 ! volume per unit area of ice (m)
&, vs1, vs2 ! volume per unit area of snow (m)
&, hi1, hi2 ! ice thickness (m)
&, hs1, hs2 ! snow thickness (m)
&, Tsf1, Tsf2 ! ice/snow top surf. temperature (K)

 real (kind=dbl_kind), intent(inout), dimension (:) ::
& ei1 ! energy of melting of ice per layer (J/m**2)
&, ei2 ! energy of melting of ice per layer (J/m**2)

4.15.11 moveup - moves ice from cat 1 to cat 2

INTERFACE:

 subroutine moveup( Tf0
$ , ai1, vi1, vs1, ei1, Tsf1
$ , hi1, hs1
& , h1min, nn1
$ , ai2, vi2, vs2, ei2, Tsf2
$ , hi2, hs2
& , h2min, nn2 )

DESCRIPTION:

Moves ice from cat 1 to 2.

It is possible that the final thickness will be above the boundary of cat 2. If the ice needs to move up again, it will do so in a subsequent call

REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& Tf0 ! temperature of ocean
&, h1min, h2min ! minimum thickness range of cat 1, 2 (m)
 integer (kind=int_kind), intent(in) ::
& nn1, nn2 ! number of layers in cat 1, 2

 real (kind=dbl_kind), intent(inout) ::
& ai1, ai2 ! fraction of ice
&, vi1, vi2 ! volume per unit area of ice (m)

&, vs1, vs2 ! volume per unit area of snow (m)
&, hi1, hi2 ! ice thickness (m)
&, hs1, hs2 ! snow thickness (m)
&, Tsf1, Tsf2 ! ice/snow top surf. temperature (K)
&, ei1(nn1) ! energy of melting of ice per layer (J/m**2)
&, ei2(nn2) ! energy of melting of ice per layer (J/m**2)

4.15.12 zerocat - reset category variables to zero when no ice

INTERFACE:

 subroutine zerocat( Tf0, ai, vi, vs, ei
$ , Tsf
& , hs, hi
& , hmin, nn )

DESCRIPTION:

Reset category variables in the case of no ice

REVISION HISTORY:

author: C. M. Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) :: Tf0 ! freezing temperature
 integer (kind=int_kind), intent(in) :: nn ! number of layers in cat
 real (kind=dbl_kind), intent(in) :: hmin

 real (kind=dbl_kind), intent(inout) ::
& ai ! fraction of ice
&, vi ! volume per unit area of ice (m)
&, vs ! volume per unit area of snow (m)
&, hi ! ice thickness (m)
&, hs ! snow thickness (m)
&, Tsf ! ice/snow top surf. temperature (K)
&, ei (nn) ! energy of melting of ice per layer (J/m**2)

4.16 Fortran: Module Interface ice itd linear - linear remapping scheme for ITD (Source File: ice itd linear.F)

Linear remapping scheme for the ice thickness distribution See Lipscomb, W. H. Remapping the thickness distribution of sea ice. 2001, J. Geophys. Res., Vol 106, 13989–14000.

REVISION HISTORY:

authors: William H. Lipscomb, LANL
         Elizabeth C. Hunke, LANL

INTERFACE:

module ice_itd_linear

USES:

use ice_model_size
use ice_kinds_mod
use ice_constants
use ice_state
use ice_itd
use shr_sys_mod, only : shr_sys_abort

4.16.1 linear itd - ITD scheme that shifts ice among categories

INTERFACE:

subroutine linear_itd(i,j,dhin,hin_old,hin,hsn)

DESCRIPTION:

Ice thickness distribution scheme that shifts ice among categories.

The default scheme is linear remapping, which works as follows. See Lipscomb (2001) for more details. Using the thermodynamic ”velocities”, interpolate to find the velocities in thickness space at the category boundaries, and compute the new locations of the boundaries. Then for each category, compute the thickness distribution function, g(h), between hL and hR, the left and right boundaries of the category. Assume g(h) is a linear polynomial that satisfies two conditions: (1) The ice area implied by g(h) equals ain(n). (2) The ice volume implied by g(h) equals ain(n)*hice(n).

Once g(h) is computed, compute the ice area and volume lying between the initial and new boundaries, and transfer this area and volume to the neighboring cell, thus restoring the initial boundary. REVISION HISTORY:

authors: William H. Lipscomb, LANL
         Elizabeth C. Hunke, LANL

USES:

use ice_domain
use ice_diagnostics
use ice_calendar

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& i,j ! grid indices
 real (kind=dbl_kind), intent(in) ::
& dhin(ncat) ! thickness change for remapping (m)
&, hin_old(ncat) ! starting value of hin (m)
 real (kind=dbl_kind), intent(inout) ::
& hin(ncat) ! ice thickness for each cat (m)
&, hsn(ncat) ! snow thickness for each cat (m)

4.16.2 fit line - fit g(h) with a line using area, volume constraints

INTERFACE:

subroutine fit_line (n, hin, Hb, g0, g1, hL, hR, i,j)

DESCRIPTION:

Fit g(h) with a line, satisfying area and volume constraints. To reduce rounding errors caused by large values of g0 and g1, we compute g(eta), where eta = h - hL. REVISION HISTORY:

authors: William H. Lipscomb, LANL
         Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& n ! thickness category for which g(h) computed
 real (kind=dbl_kind), intent(in) ::
& hin(ncat) ! ice thickness for each cat (m)
&, Hb(0:ncat) ! current category boundaries
 real (kind=dbl_kind), intent(out) ::
& g0, g1 ! coefficients in linear equation for g(eta)
&, hL ! min value of range over which g(h) > 0
&, hR ! max value of range over which g(h) > 0
 integer (kind=int_kind), intent(in) ::
& i,j

4.16.3 shift ice - shift ice across category boundaries

INTERFACE:

subroutine shift_ice (donor, daice, dvice, hin, i,j)

DESCRIPTION:

Shift ice across category boundaries, conserving area, volume, and energy. REVISION HISTORY:

authors: William H. Lipscomb, LANL
         Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) ::
& donor(ncat-1) ! donor category index

 real (kind=dbl_kind), intent(inout) ::
& daice(ncat-1) ! ice area transferred across boundary
&, dvice(ncat-1) ! ice volume transferred across boundary

 real (kind=dbl_kind), intent(in) ::
& hin(ncat) ! ice thickness for each cat (m)

 integer (kind=int_kind), intent(in) ::
& i,j

4.17 Fortran: Module Interface ice kinds mod - defines variable precision (Source File: ice kinds mod.F)

Defines variable precision for all common data types Code originally based on kinds mod.F in POP

REVISION HISTORY:

author: Elizabeth C. Hunke
       Fluid Dynamics Group, Los Alamos National Laboratory

INTERFACE:

module ice_kinds_mod

USES:

4.18 Fortran: Module Interface ice mechred - computes mech redistribution and strength for ITD (Source File: ice mechred.F)

Ice thickness distribution model with multi-layer thermodynamics. Routines to compute mechanical redistribution and strength.

See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669-15,677.

See Bitz, C.M., M.M. Holland, A.J. Weaver, M. Eby, 2001: Simulating the ice-thickness distribution in a climate model, J. Geophys. Res., 106, 2441–2464.

REVISION HISTORY:

author: C. M. Bitz

INTERFACE:

module ice_mechred

USES:

use ice_model_size
use ice_constants
use ice_state
use ice_itd
use ice_dyn_evp

4.18.1 init mechred - initialize constants for ridging

INTERFACE:

subroutine init_mechred

DESCRIPTION:

Initialize constants for ridging REVISION HISTORY:

author: C.M.Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

4.18.2 mechanical redistr - driver for ridging

INTERFACE:

subroutine mechanical_redistr

DESCRIPTION:

This routine works with ncat=1 In fact, it will provide a source of open water from shear deformation. See Stern et al, 1995 for information about how and why this is done Keeps track of heat and fresh water flx to ocn if snow on ice that ridges is thrown into the ocean

REVISION HISTORY:

author: C.M.Bitz, UW

USES:

use ice_domain
use ice_flux
use ice_grid
use ice_timers
use ice_calendar, only: dt

INPUT/OUTPUT PARAMETERS:

4.18.3 ridge - ridge ice due to convergence or shear deformation

INTERFACE:

 subroutine ridge( dt1, closng, epsi, delta_local, Tf1,
$ Fhnet1, Fresh1, Gamm, H2Gamm)

DESCRIPTION:

Ridge ice due to convergence or shear deformation note the timestep is dt1 for ridging among the cats however will subcycle with timestep dtsub if a cat would run out of ice if the timestep were greater than dtsub Throw snow on ice that ridges into ocean if snow into ocn=.true.

REVISION HISTORY:

author: C.M.Bitz, UW

USES:

use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& dt1
&, delta_local ! Delta from dynamics routine
&, Tf1 ! ocean freezing temperature
 real (kind=dbl_kind), intent(out) ::
& Fhnet1 ! heat given to ocean from snow (N/m)
&, Fresh1 ! water given to ocean from snow (m)
&, H2Gamm (ncat,ncat) ! H*volume frac from cat i that goes into j
 real (kind=dbl_kind), intent(inout) ::
& Gamm (ncat,ncat) ! area frac from cat i that goes into j
&, epsi ! actual divergence computed from transport (1/s)
&, closng ! closing from Flato & Hibler Eq. 9 (1/s)

4.18.4 ridging mode - compute W and Wa factors

INTERFACE:

subroutine ridging_mode( W, Wa, Gamm )

DESCRIPTION:

Compute W and Wa, factors for ridging mode and participation function REVISION HISTORY:

author: C.M.Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& Gamm (ncat,ncat) ! area frac from cat i that goes into j
 real (kind=dbl_kind), intent(out) ::
& W (0:ncat) ! W factor, geometric comp. of ridging mode
&, Wa (0:ncat) ! part of W from participation func.

4.18.5 ridge matrices - compute Gamma factors

INTERFACE:

subroutine ridge_matrices( hin, Hmean, Gamm, HGamm, H2Gamm )

DESCRIPTION:

Compute Gamm,HGamm,H2Gamm for ridge and strength for true thicknesses REVISION HISTORY:

author: C.M.Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(out) ::
& hin (ncat) ! ice thickness (m)
&, Hmean (ncat) ! mean thickness of ridg ice from cat nc (m)
&, Gamm (ncat,ncat) ! area frac from cat i that goes into j
&, HGamm (ncat,ncat) ! volume frac from cat i that goes into j
&, H2Gamm (ncat,ncat) ! H*volume frac from cat i that goes into j
  ! HGamm is used in ridge and H2Gamm is used in roth_strength

4.18.6 comp matrices - compute Gamm functions

INTERFACE:

 subroutine comp_matrices( rowflg, hin, Hmean,
$ Gamm, HGamm, H2Gamm )

DESCRIPTION:

Compute Gamm, HGamm, H2Gamm HGamm is used in ridge and H2Gamm is used in roth-strength Gamm(nc,k) distributes ice that participates in ridging from cat nc into a distrib. of cats k n1 is the smallest k with nonzero fract n2 is the largest k with nonzero fract ice that partic. has thickness hin(nc) and it ridges up to linear distrib. between 2*hin(nc) and 2*sqrt(cK*hin(nc)) REVISION HISTORY:

author: C.M.Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 logical (kind=log_kind), intent(in) ::
& rowflg(ncat) ! true if cat has nonzero fractional area
 real (kind=dbl_kind), intent(in) ::
& hin (ncat) ! ice thickness (m)

 real (kind=dbl_kind), intent(out) ::
& Hmean (ncat) ! mean thickness of ridg ice from cat nc (m)
&, Gamm (ncat,ncat) ! area frac from cat i that goes into j
&, HGamm (ncat,ncat) ! volume frac from cat i that goes into j
&, H2Gamm (ncat,ncat) ! H*volume frac from cat i that goes into j

4.18.7 real function roth strength - Rothrock ice strength

INTERFACE:

real function roth_strength( Gamm ,H2Gamm )

DESCRIPTION:

Compute the ice strength based on Rothrock, 1975 and also see FH95 does not make sense to do this unless the ice that participates in ridging is well resolved – must have about 5 categories, 10 would be better REVISION HISTORY:

author: C.M.Bitz, UW

USES:

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind), intent(in) ::
& Gamm (ncat,ncat) ! area frac from cat i that goes into j
&, H2Gamm (ncat,ncat) ! H*volume frac from cat i that goes into j

4.19 Fortran: Module Interface ice model size - defines global domain size, category and layer number (Source File: ice model size.F)

Defines the global domain size and number of categories and layers. Code originally based on model size.F in POP REVISION HISTORY:

author Elizabeth C. Hunke
       Fluid Dynamics Group, Los Alamos National Laboratory

INTERFACE:

module ice_model_size

USES:

use ice_kinds_mod

4.20 Fortran: Module Interface ice mpi internal - parameters and common blocks for MPI internal to ice model (Source File: ice mpi internal.F)

Parameters and commons blocks for MPI parallelization internal to ice model REVISION HISTORY:

authors: Tony Craig, NCAR
         Elizabeth C. Hunke, LANL

INTERFACE:

module ice_mpi_internal

USES:

use ice_kinds_mod
use ice_domain

4.20.1 ice global real minmax - computes global min/max and prints

INTERFACE:

subroutine ice_global_real_minmax(nc,work,string)

DESCRIPTION:

Determines and writes both minimum and maximum over global grid REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nc
real (kind=dbl_kind), intent(in) :: work(nc)
character (len=8), intent(in) :: string

4.20.2 real function ice global real minval - computes global min

INTERFACE:

real function ice_global_real_minval(nc,work)

DESCRIPTION:

Computes minimum over the global grid REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nc
real (kind=dbl_kind), intent(in) :: work(nc)

4.20.3 real function ice global real maxval - computes global max

INTERFACE:

real function ice_global_real_maxval(nc,work)

DESCRIPTION:

Computes maximum over the global grid REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nc
real (kind=dbl_kind), intent(in) :: work(nc)

4.20.4 real function ice global real sum - sums input array over global grid

INTERFACE:

real function ice_global_real_sum(nc,work)

DESCRIPTION:

Sums given array over the global grid REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nc
real (kind=dbl_kind), intent(in) :: work(nc)

4.20.5 ice bcast logical - broadcasts scalar logical to all processors

INTERFACE:

subroutine ice_bcast_logical(logval)

DESCRIPTION:

Broadcasts a scalar logical value to all processors REVISION HISTORY:

author: Julie Schramm, NCAR
        Added 22 Oct 2001

USES:

INPUT/OUTPUT PARAMETERS:

implicit none
logical (kind=log_kind), intent(inout) :: logval

4.20.6 ice bcast char - broadcasts scalar character to all processors

INTERFACE:

subroutine ice_bcast_char(charval)

DESCRIPTION:

Broadcasts a scalar character value to all processors REVISION HISTORY:

author: Julie Schramm, NCAR
        Added 22 Oct 2001

USES:

INPUT/OUTPUT PARAMETERS:

implicit none
character (*), intent(inout) :: charval

4.20.7 ice bcast rscalar - broadcasts real scalar all processors

INTERFACE:

subroutine ice_bcast_rscalar(val)

DESCRIPTION:

Broadcasts a real scalar character value to all processors REVISION HISTORY:

author: Julie Schramm, NCAR
        Added 22 Oct 2001

USES:

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind), intent(inout) :: val

4.20.8 ice bcast iscalar - broadcasts integer scalar all processors

INTERFACE:

subroutine ice_bcast_iscalar(ival)

DESCRIPTION:

Broadcasts an integer scalar character value to all processors REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(inout) :: ival

4.20.9 global scatter - scatters global to distributed array, adding ghost cells

INTERFACE:

subroutine global_scatter(workg,work)

DESCRIPTION:

Scatters a global array and adds ghost cells to create a distributed array REVISION HISTORY:

author: Tony Craig, NCAR

USES:

use ice_model_size
use ice_constants

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind) :: workg(imt_global,jmt_global)
&, work(ilo:ihi,jlo:jhi)

4.20.10 global gather - gathers distributed array into global array

INTERFACE:

subroutine global_gather(workg,work)

DESCRIPTION:

Gathers a distributed array and strips off ghost cells to create a local array with global dimensions REVISION HISTORY:

author: Tony Craig, NCAR

USES:

use ice_model_size
use ice_constants

INPUT/OUTPUT PARAMETERS:

 real (kind=dbl_kind) :: workg(imt_global,jmt_global)
&, work(ilo:ihi,jlo:jhi)

4.20.11 get sum - computes weighted sum over global grid

INTERFACE:

subroutine get_sum(flag,work1,work2,work3,gsum)

DESCRIPTION:

Computes a (weighted) sum over the global grid; if flag = 1 then work1 is weighted by work2 before being added to work3 REVISION HISTORY:

author: Elizabeth C. Hunke, LANL

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: flag
 real (kind=dbl_kind), intent(in) ::
& work1(ilo:ihi,jlo:jhi)
&, work2(ilo:ihi,jlo:jhi)
 real (kind=dbl_kind), intent(in) ::
& work3(imt_local,jmt_local)
 real (kind=dbl_kind), intent(out) ::
& gsum

4.20.12 end run - ends run

INTERFACE:

subroutine end_run

DESCRIPTION:

Ends run by calling MPI FINALIZE. REVISION HISTORY:

author: ?

USES:

INPUT/OUTPUT PARAMETERS:

#ifdef _MPI
      call MPI_FINALIZE(ierr)
#endif

4.21 Fortran: Module Interface ice ocean - ocean mixed layer internal to sea ice model (Source File: ice ocean.F)

Ocean mixed layer calculation (internal to sea ice model).

Open ocean has stability based flux calculations for uncoupled runs. Uses monthly mean ocean forcing data from external file to drive the ocean mixed layer. Initial sst either from the ice restart file or set to 1 Jan from external file data./initial

List of ocean forcing fields: Note that order is important! (order is determined by field list in vname). For ocean mixed layer—————————–units 1 sst——temperature—————————(C) 2 sss——salinity——————————(ppt) 3 hbl——depth———————————(m) 4 u——–surface u current———————(m/s) 5 v——–surface v current———————(m/s) 6 dhdx—–surface tilt x direction————–(m/m) 7 dhdy—–surface tilt y direction————–(m/m) 8 qdp——ocean sub-mixed layer heat flux——-(W/m2)

REVISION HISTORY:

original authors John Weatherly, C.M. Bitz,
                 Elizabeth C. Hunke, Bruce P. Briegleb
significantly modified by Bruce P. Briegleb

INTERFACE:

module ice_ocean

USES:

use ice_flux
use ice_calendar
use ice_prnpnt

4.21.1 init oceanmixed ice - initialize mixed layer forcing data

INTERFACE:

subroutine init_oceanmixed_ice

DESCRIPTION:

Initialize ocean forcing data for the mixed layer. Check netCDF file for correct dimensions, fields and other attributes, and then read in all 12 months of forcing data.

Assumes 12 months of ocean forcing data, ordered from mean January to mean December; dates of these months are ignored.

Note the assumption that if lat/lon dimensions of the netCDF files are identical to those in the code, then the grids of the netCDF file and the code are also.

REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use ice_mpi_internal
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort
include "netcdf.inc"

INPUT/OUTPUT PARAMETERS:

4.21.2 time intrplt ocean forcing - time interpolates ocean forcing

INTERFACE:

subroutine time_intrplt_ocean_forcing

DESCRIPTION:

Finds two months of ocean forcing data that bracket current date (for which year is ignored), and interpolate linearly in time between those two values. REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use ice_mpi_internal
use ice_grid
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort
include "netcdf.inc"

INPUT/OUTPUT PARAMETERS:

4.21.3 set oceanmixed ice - set sst and frzmlt

INTERFACE:

subroutine set_oceanmixed_ice

DESCRIPTION:

Sets sst and frzmlt with ocean mixed layer values REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use shr_sys_mod, only : shr_sys_flush

INPUT/OUTPUT PARAMETERS:

4.21.4 compute oceanmixed ice - update ocean state fields

INTERFACE:

subroutine compute_oceanmixed_ice

DESCRIPTION:

Update sst and other ocean state fields REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use shr_sys_mod, only : shr_sys_flush

INPUT/OUTPUT PARAMETERS:

4.21.5 mixed layer(i,j) - computes open ocean fluxes

INTERFACE:

subroutine mixed_layer(i,j)

DESCRIPTION:

Calculate flux exchange over open ocean and update mixed layer sst REVISION HISTORY:

author Elizabeth Hunke, LANL, and Bruce P. Briegleb, NCAR

USES:

use ice_grid
use ice_atmo
use ice_constants, only : TTTocn, qqqocn

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: i,j

4.21.6 ocnheat(i,j, delt, delq) - update ocean fields

INTERFACE:

subroutine ocnheat(i,j, delt, delq)

DESCRIPTION:

Update sst and freezing/melting potential; set other ocean fields from forcing data; thermal effect of ice/ocn heat will be included in the sst change after this routine is called. REVISION HISTORY:

Modified by Bruce P. Briegleb

USES:

use ice_constants
use ice_state
use ice_albedo

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind) :: i,j
 real (kind=dbl_kind), intent(in) ::
& delt ! potential T difference (K)
&, delq ! humidity difference (kg/kg)

4.22 Fortran: Module Interface ice prescribed - Prescribed Ice (Source File:

ice prescribed.F)

Prescribed ice.

Set ice concentration with prescribed data from netCDF data file; then internally prescribe ice thickness, temperature, snow cover, layer linear temperature profile; finally, compute air/ice fluxes, but no other ice thermo or dynamics; set ice/ocean fluxes to zero. REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

INTERFACE:

module ice_prescribed

USES:

use ice_model_size
use ice_constants
use ice_domain
use ice_grid
use ice_calendar

4.22.1 init prescribed ice - initialize prescribed ice data

INTERFACE:

subroutine init_prescribed_ice

DESCRIPTION:

Initialize climatological ice concentration data by checking existing netCDF file for correct dimensions, fields and other attributes, and then reading in first 12 months of ice cover data for climatology case and 2 months (12 and 13) for non-climatology.

Note the assumption that if lat/lon dimensions of the netCDF files are identical to those in the code, then the grids of the netCDF file and the code are also. REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

USES:

use ice_mpi_internal
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.22.2 read prescribed ice - read in two ice concentration fields

INTERFACE:

subroutine read_prescribed_ice

DESCRIPTION:

Read in two ice concentration fields that bracket current date, and interpolate linearlly in time between those two values. Make sure final ice concentration exceeds a small constant value. No time extrapolation allowed; if date out of range, exit. Data may have values ¡ 0 or ¿ 1; limit 1.0e-4 to 1 after time interpolation. REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

USES:

use ice_mpi_internal
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.22.3 read prescribed ice climate - read two climate ice concentrations

INTERFACE:

subroutine read_prescribed_ice_climate

DESCRIPTION:

Finds two months of climatological ice concentration that bracket current date (for which year is ignored), and interpolate linearlly in time between those two values. Final time inerpolated ice concentration is limited to the range 1.0e-4 to 1. REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

USES:

use ice_mpi_internal
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.22.4 set prescribed ice state - set prescribed ice state

INTERFACE:

subroutine set_prescribed_ice_state

DESCRIPTION:

Set prescribed ice state using input ice concentration; set snow to specified value; set surface ice temperature to atmospheric value; use linear temperature gradient in ice to ocean temperature. REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

USES:

use ice_flux
use ice_vthermo
use ice_state
use ice_itd
use ice_dh
use shr_sys_mod, only : shr_sys_flush, shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.22.5 set prescribed ice flux - Set non-computed fluxes to zero

INTERFACE:

subroutine set_prescribed_ice_flux

DESCRIPTION:

Set non-computed fluxes for prescribed ice model to zero REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

USES:

use ice_dyn_evp
use ice_flux

INPUT/OUTPUT PARAMETERS:

4.22.6 exit prescribed ice - close netCDF file for prescribed ice

INTERFACE:

subroutine exit_prescribed_ice

DESCRIPTION:

Close netCDF file for prescribed ice REVISION HISTORY:

author: Bruce P. Briegleb, NCAR

INPUT/OUTPUT PARAMETERS:

4.23 Fortran: Module Interface ice prnpnt - diagnostic grid point info during execution (Source File: ice prnpnt.F)

This module defines the grid points desired for printout of atmospheric and ocean inputs and ice model outputs. Data for each point is written to a separate file as ascii tables. The specific points are set by lat/lons (-90 to 90 lat and -180 to +180 lon) in a data statement. A descriptive label is useful to distinguish points. The code chooses the nearest model grid point to the specified lat/lon. Points for task 0 are written in the ice model execution directory; all other task points are written one directory up (on IBM). REVISION HISTORY:

author Bruce P. Briegleb, NCAR

INTERFACE:

module ice_prnpnt

USES:

use ice_domain
use ice_constants
use ice_calendar
use shr_sys_mod, only : shr_sys_flush

4.23.1 intpnt - initializes printout of grid point data

INTERFACE:

subroutine intpnt

DESCRIPTION:

Initialize printout of points by finding tasks for requested points, and defining file names for each point. Prints out description of points and tasks to log file. REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use ice_grid
use ice_mpi_internal

INPUT/OUTPUT PARAMETERS:

4.23.2 diags cpl in - grid point printout of input info from coupler

INTERFACE:

subroutine diags_cpl_in

DESCRIPTION:

Printout atmospheric forcing data for selected grid points as received from the coupler. REVISION HISTORY:

author Bruce P. Briegleb, NCAR

USES:

use ice_flux
use ice_calendar

INPUT/OUTPUT PARAMETERS:

4.23.3 diags cpl out - grid point printout of info sent to coupler

INTERFACE:

subroutine diags_cpl_out

DESCRIPTION:

Printout grid point info sent to coupler USES:

use ice_flux
use ice_albedo
use ice_calendar
use ice_state

INPUT/OUTPUT PARAMETERS:

4.24 Fortran: Module Interface ice read write - routines for opening, reading and writing external files (Source File: ice read write.F)

Routines for opening, reading and writing external files REVISION HISTORY:

author: Tony Craig, NCAR

INTERFACE:

module ice_read_write

USES:

use ice_model_size
use ice_domain
use ice_mpi_internal

4.24.1 ice open - opens an unformatted file for reading

INTERFACE:

subroutine ice_open(nu,filename,nbits)

DESCRIPTION:

Opens an unformatted file for reading nbits indicates whether the file is sequential or direct access REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nu,nbits
character (*) :: filename

4.24.2 ice read - reads an unformatted file

INTERFACE:

subroutine ice_read(nu,nrec,work,atype,scatter)

DESCRIPTION:

Reads an unformatted file work is a real array, atype indicates the format of the data REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nu,nrec
real (kind=dbl_kind) :: work(ilo:ihi,jlo:jhi)
character (len=4) atype ! real,int
logical (kind=log_kind) :: scatter

4.24.3 ice write - writes an unformatted file

INTERFACE:

subroutine ice_write(nu,nrec,work,atype,gather)

DESCRIPTION:

Writes an unformatted file work is a real array, atype indicates the format of the data REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: nu,nrec
real (kind=dbl_kind) :: work(ilo:ihi,jlo:jhi)
character (len=4) atype ! real,int
logical (kind=log_kind) :: gather

4.25 Fortran: Module Interface ice scaling - scale ice (Source File: ice scaling.F)

INTERFACE:

module ice_scaling

REVISION HISTORY:

author: C.M.Bitz ?

USES:

use ice_domain
use ice_kinds_mod
use ice_constants
use ice_state

4.25.1 scale fluxes - scale fluxes

INTERFACE:

subroutine scale_fluxes

REVISION HISTORY:

author: C.M.Bitz ?

USES:

use ice_flux
use ice_albedo
use ice_history
use ice_grid

INPUT/OUTPUT PARAMETERS:

4.25.2 scale hist fluxes - scale history fluxes

INTERFACE:

subroutine scale_hist_fluxes

REVISION HISTORY:

author: C.M.Bitz ?

USES:

use ice_flux
use ice_albedo
use ice_history
use ice_grid

INPUT/OUTPUT PARAMETERS:

4.26 Fortran: Module Interface ice state - primary state variables (Source File:

ice state.F)

Primary state variables in various configurations Note: other state variables are at the end of this... The primary state variable names are:

main——single-column–single column,—aggregated—units ——————————–single category—over cats

aicen(i,j,n)—ain(n)———ai————–aice(i,j)——— vicen(i,j,n)—vin(n)——–vi or hi——–vice(i,j)——m vsnon(i,j,n)—vsn(n)——–vs or hs——–vsno(i,j)——m eicen(i,j,k)—ein(k,n)——-ei(k)———–eice(i,j)——J/m2 Tsfcn(i,j,n)—Tsfn(n)——-Tsf————-Tsfc(i,j)——deg

Area is dimensionless because aice is the fractional area (normalized so that the sum over all categories, including open water, is one). That is why vice/vsno have units of m instead of m3, and eice/esno have units of J/m2 instead of J.

Note that variable names follow 2 simple rules:

(1) If a variable has dimensions i and j, write ’ice’ or ’sno’ or ’sfc’; else abbreviate as ’i’ or ’s’ or ’sf’. (2) If a variable has dimension n, add an ’n’; else omit the ’n’.

We will also use the variables hice = vice/aice, hsno = vsno/aice, qice = eice/vice, and qsno = esno/vsno. These variables will follow the same naming convention. They will not be state variables but will be computed as needed in individual subroutines.

REVISION HISTORY:

authors C. M. Bitz, UW
        Elizabeth C. Hunke, LANL

INTERFACE:

module ice_state

USES:

use ice_kinds_mod
use ice_model_size
use ice_domain

4.27 Fortran: Module Interface ice therm driver - driver for thermodynamics and itd (Source File: ice therm driver.F)

Energy-conserving sea ice model Driver for thermodynamics and associated changes to the itd

See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669-15,677.

See Bitz, C.M., M.M. Holland, A.J. Weaver, M. Eby, 2001: Simulating the ice-thickness distribution in a climate model, J. Geophys. Res., 106, 2441–2464.

REVISION HISTORY:

author C. M. Bitz
code heavily modified by Elizabeth C. Hunke, LANL

INTERFACE:

module ice_therm_driver

USES:

use ice_kinds_mod
use ice_model_size
use ice_constants
use ice_state
use ice_flux
use ice_diagnostics
use ice_calendar

4.27.1 thermo rates - compute thermo growth rates and atm fluxes

INTERFACE:

subroutine thermo_rates

DESCRIPTION:

compute thermodynamic growth rates and atmospheric fluxes REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_domain
use ice_timers
use ice_vthermo
use ice_grid
use ice_itd
use ice_init

INPUT/OUTPUT PARAMETERS:

4.27.2 thermo itd - changes in itd due to thermodynamic growth

INTERFACE:

subroutine thermo_itd

DESCRIPTION:

Changes to ice thickness distribution associated with thermodynamic growth rates, including lateral growth/melt NOTE: ocean fluxes are initialized here REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_domain
use ice_timers
use ice_history
use ice_grid
use ice_itd
use ice_itd_linear
use ice_init

INPUT/OUTPUT PARAMETERS:

4.27.3 init column diags - initialize column diagnostics

INTERFACE:

subroutine init_column_diags(i,j,hfatm)

DESCRIPTION:

initialize diagnostic and history variables REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_history

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind) :: i, j
 real (kind=dbl_kind), intent(out) ::
& hfatm ! heat flx to ice-snow from atm (J/m**2)

4.27.4 init vertical profile - initialize vertical ice profile

INTERFACE:

subroutine init_vertical_profile(i,j,ei0,hin,hsn,tiz)

DESCRIPTION:

initialize the vertical profile of ice properties REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_vthermo
use ice_itd

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j
 real (kind=dbl_kind), intent(out) ::
& ei0 ! initial energy in ice/snow (J/m**2)
&, hin(ncat) ! ice thickness for each cat (m)
&, hsn(ncat) ! snow thickness for each cat (m)
&, tiz(0:nmax,ncat) ! temp of each layer for each cat (C)

4.27.5 init frzmlt - initialize ocean-ice heat fluxes, bottom and lateral

INTERFACE:

subroutine init_frzmlt(i,j,Fbot,Fnew,Rside)

DESCRIPTION:

Initialize ocean-ice heat fluxes: bottom and lateral Assuming frzmlt is per grid box area REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_itd

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i, j
 real (kind=dbl_kind), intent(out) ::
& Fbot ! heat flx to ice bottom, (W/m**2)
&, Fnew ! heat flx to open water, (W/m**2)
&, Rside ! fraction of ice that melts from side

4.27.6 lateral growth melt - frazil ice growth and lateral melt

INTERFACE:

subroutine lateral_growth_melt(i,j,Fnew,Rside,hin)

DESCRIPTION:

frazil ice growth / lateral melt REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_vthermo
use ice_history
use ice_itd

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j
 real (kind=dbl_kind), intent(in) ::
& Fnew ! heat flx to open water (W/m**2)
&, Rside ! fraction of ice that melts from side
 real (kind=dbl_kind), intent(inout) ::
& hin(ncat) ! ice thickness for each cat (m)

4.27.7 reduce area - reduce area when ice melts for special case ncat=1

INTERFACE:

subroutine reduce_area(i,j,dhi1,hin,hsn)

DESCRIPTION:

Reduce area when ice melts for special case of ncat=1 Use CSM 1.0-like method of reducing ice area when melting occurs: assume only half the ice volume change goes to thickness decrease, the other half to reduction in ice fraction REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_kinds_mod
use ice_constants
use ice_flux !! not necessary if rebin is called instead
use ice_state
use ice_itd

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i,j
 real (kind=dbl_kind), intent(in) ::
& dhi1 ! melt at bottom and top plus sublimation (m)
 real (kind=dbl_kind), intent(inout) ::
& hin(ncat) ! ice thickness for each cat (m)
&, hsn(ncat) ! ice thickness for each cat (m)

4.27.8 conservation check - enforce ice property conservation

INTERFACE:

subroutine conservation_check(i,j,ei0,hfatm,hfocn)

DESCRIPTION:

Make sure ice properties are properly conserved REVISION HISTORY:

authors: C.M.Bitz (UW)
modified by: E.C.Hunke (LANL).

USES:

use ice_itd

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i, j

 real (kind=dbl_kind), intent(in) ::
& ei0 ! initial energy in ice/snow (J/m**2)
&, hfatm ! heat flx to ice-snow from atm (J/m**2)
&, hfocn ! heat flx to ice-snow from ocn (J/m**2)

4.28 Fortran: Module Interface ice timers (Source File: ice timers.F)

Timing routines REVISION HISTORY:

author: Tony Craig, NCAR

INTERFACE:

module ice_timers

DESCRIPTION:

Timing routines REVISION HISTORY:

author: Tony Craig, NCAR

USES:

use ice_kinds_mod
use ice_constants
implicit none

4.28.1 ice timer clear(n) - initialize timer n to 0

INTERFACE:

subroutine ice_timer_clear(n)

DESCRIPTION:

Initialize timer n to 0 if n = -1 initialize all timers REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: n

4.28.2 ice timer start(n) - begin timing with timer n

INTERFACE:

subroutine ice_timer_start(n)

DESCRIPTION:

Begin timing with timer n REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: n

4.28.3 ice timer stop(n) - end (or pause) timing with timer n

INTERFACE:

subroutine ice_timer_stop(n)

DESCRIPTION:

End (or pause) timing with timer n REVISION HISTORY:

author: Tony Craig, NCAR

USES:

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: n

4.28.4 ice timer print(n) - print timing results of timer n

INTERFACE:

subroutine ice_timer_print(n)

DESCRIPTION:

Print timing results of timer n if n = -1 print timing results of all timers REVISION HISTORY:

author: Tony Craig, NCAR

USES:

use ice_domain
use ice_mpi_internal

INPUT/OUTPUT PARAMETERS:

integer (kind=int_kind), intent(in) :: n

4.28.5 timers(t1) - do the work

INTERFACE:

subroutine timers(t1)

DESCRIPTION: Do the work REVISION HISTORY:

author: Tony Craig, NCAR

USES:

#ifdef _MPI
      include "mpif.h" ! MPI library definitions
#else
#ifdef Linux
      integer (kind=int_kind) ::
     & count ! current count of the system clock
     &, count_rate ! number of clock ticks per second
#else
      real (kind=dbl_kind) :: rtc
      integer (kind=int_kind) :: rate,irtc_rate
#endif
#endif

INPUT/OUTPUT PARAMETERS:

real (kind=dbl_kind), intent(out) :: t1

4.29 Fortran: Module Interface ice transport - horizontal advection (via mpdata) (Source File: ice transport.F)

Calculates horizontal advection using mpdata (Multidimensional Positive Definite Advection Transport Algorithm).

REVISION HISTORY:

author Elizabeth C. Hunke

INTERFACE:

module ice_transport

USES:

use ice_model_size
use ice_domain
use ice_constants
use ice_grid

4.29.1 transport - computes transport equations for one timestep

INTERFACE:

subroutine transport

DESCRIPTION:

Computes the transport equations for one timestep using mpdata. Sets several fields into a work array and passes it to mpdata routine. REVISION HISTORY:

author Elizabeth C. Hunke

USES:

use ice_flux
use ice_timers
use ice_state

INPUT/OUTPUT PARAMETERS:

4.29.2 mpdata(narrays,phi) - advection according to mpdata

INTERFACE:

subroutine mpdata(narrays,phi)

DESCRIPTION:

Smolarkiewicz, P. K., 1984: A fully multidimensional positive definite advection transport algorithm with small implicit diffusion, J. Comput. Phys., 54, 325-362. REVISION HISTORY:

author Elizabeth C. Hunke

USES:

use ice_calendar
use ice_dyn_evp
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: narrays
 real (kind=dbl_kind), intent(inout) ::
& phi(imt_local,jmt_local,narrays)

4.30 Fortran: Module Interface ice tstm - energy conserving sea ice model thermodynamics (Source File: ice tstm.F)

Energy-conserving sea ice model Routines to solve heat-equation using linear method

See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669-15,677.

See Bitz, C.M., M.M. Holland, A.J. Weaver, M. Eby, 2001: Simulating the ice-thickness distribution in a climate model, J. Geophys. Res., 106, 2441–2464.

REVISION HISTORY:

author: C. M. Bitz

INTERFACE:

module ice_tstm

USES:

use ice_constants
use ice_itd

4.30.1 tstm - calculates surface and internal snow/ice temp

INTERFACE:

 subroutine tstm( dtau, tmz1d, sal1d, Tf1
$ , area, hi, hs, dswr
$ , dswrv, dswrn, flwd, dflwup
$ , dflh, dfsh, asnow, ni
$ , tbot, Ib, F, condb
$ , ts, ti, flwup, flh
$ , fsh)

DESCRIPTION:

This routine calculates the evolution of the ice interior and surface temperature from the heat equation and surface energy balance

The albedo is fixed for this calculation

Solves the heat equation which is non-linear for saline ice by linearizing and then iterating a set of equations Scheme is backwards Euler giving a tridiagonal set of equations implicit in temperature (Tried crank-nicholson but it behaves poorly when thin ice has a weird initial temperature profile.

NOTE there are two values for minimum snow thickness, hs-min used elsewhere in the code, and hsmin used here. CC says:

The solution to the heat equation ignores the insulating effect of snow if it less than 0.01 m thick, but I do not like to ”kill” it when it is that thick because sometimes the snowfall rate is really small... Must have a sufficient amount of snow to solve heat equation in snow hsmin is the minimum depth of snow in order to solve for ti(0) if snow thickness is less than hsmin then do not change ti(0)

The number of equations that must be solved by the tridiagonal solver depends on whether the surface is melting and whether there is snow. Four cases are possible:

1 = freezing w/ snow, 2 = freezing w/ no snow, 3 = melting w/ snow, and 4 = melting w/ no snow

REVISION HISTORY:

author: C. M. Bitz

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: ni ! number vertical layers in ice
 real (kind=dbl_kind), intent(in) ::
& dtau ! timestep (s)
&, tmz1d(ni)! melting temp of each layer (C)
&, sal1d(ni+1) ! salinity of each layer (ppt)
&, area ! area of the ice/snow
&, hi,hs ! ice and snow thickness (m)
&, asnow ! 1 - patchy snow frac
&, dswr ! above srfc net dnwd shortwave, positive down (W/m**2)
&, dswrv ! dswr in vis (wvlngth < 700nm) (W/m**2)
&, dswrn ! dswr in nir (wvlngth > 700nm) (W/m**2)
&, flwd ! dnwd longwave flux (always positive) (W/m**2)
&, dfsh ! derriv wrt ts of dnwd sensible flux (W/m**2)
&, dflh ! derriv wrt ts of dnwd latent flux (W/m**2)
&, dflwup ! derriv wrt ts of upwd longwave flux (W/m**2)
&, Tf1 ! freezing temp of water below ice (C)

 real (kind=dbl_kind), intent(out) ::
& tbot ! bottom ice temp (C)
&, condb ! conductive flux at bottom srfc (W/m**2)
&, F ! net flux at top srfc including conductive flux (W/m**2)
&, Ib ! solar passing through the bottom ice srfc (W/m**2)

 real (kind=dbl_kind), intent(inout) ::
& ts ! srfc temp of snow or ice (C)
&, ti(0:ni) ! snow(0) and ice(1:ni) interior temp (C)
&, fsh ! dnwd sensible flux (W/m**2)
&, flh ! dnwd latent flux (always negative) (W/m**2)
&, flwup ! upwd longwave flux (always negative) (W/m**2)

4.30.2 getabc - computes elements of tridiagonal matrix

INTERFACE:

subroutine getabc(a,b,c,r,ti,tbot,zeta,k,eta,ni,lfirst)

DESCRIPTION:

Compute elements of tridiagonal matrix

REVISION HISTORY:

author: C. M. Bitz

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: ni ! number of layers
$ ,lfirst ! start with this layer
 real (kind=dbl_kind), intent(in) ::
& ti (0:ni) ! temperature of ice-snow layers
$ ,tbot ! temperature of ice bottom srfc
$ ,zeta (0:nmax) !
$ ,k (0:nmax+1) ! ice-snow conductivitiy
$ ,eta (0:nmax) !
 real (kind=dbl_kind), intent(out) ::
& a (-1:nmax) ! sub-diagonal elements
$ ,b (-1:nmax) ! diagonal elements
$ ,c (-1:nmax) ! super-diagonal elements
$ ,r (-1:nmax) ! constants (indep. of ti)

4.30.3 tridag - solves tridiagonal equations

INTERFACE:

subroutine tridag(a,b,c,r,u,ni)

DESCRIPTION:

Solves tridiagonal equations REVISION HISTORY:

author: C. M. Bitz

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: ni ! number of rows
 real (kind=dbl_kind), intent(in) ::
& a (nmax) ! sub-diagonal elements
$ ,b (nmax) ! diagonal elements
$ ,c (nmax) ! super-diagonal elements
$ ,r (nmax) ! constants (indep. of ti)
 real (kind=dbl_kind), intent(out) ::
& u (nmax) ! solution

4.30.4 conductiv - calculates T,S dependent conductivity

INTERFACE:

subroutine conductiv(sal1d,hsmin,ki,ti,tbot,hs,dhi,ni)

DESCRIPTION:

Calculates T,S dependent conductivity REVISION HISTORY:

author: C. M. Bitz

USES:

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: ni ! number of layers
 real (kind=dbl_kind), intent(in) ::
& hsmin ! minimum allowable snow thickness for heat eq.
&, sal1d(ni+1) ! salinity of each layer
&, hs,ti(0:ni),tbot,dhi
 real (kind=dbl_kind), intent(out) ::
& ki(0:nmax+1)

4.31 Fortran: Module Interface ice vthermo - main routines for energy-conserving vertical thermodynamics (Source File: ice vthermo.F)

Energy-conserving sea ice model Main routines for vertical thermodynamics See Bitz, C.M., and W.H. Lipscomb, 1999: An energy-conserving thermodynamic model of sea ice, J. Geophys. Res., 104, 15,669-15,677.

See Bitz, C.M., M.M. Holland, A.J. Weaver, M. Eby, 2001: Simulating the ice-thickness distribution in a climate model, J. Geophys. Res., 106, 2441–2464.

REVISION HISTORY:

author C. M. Bitz

INTERFACE:

module ice_vthermo

USES:

use ice_model_size
use ice_domain
use ice_constants
use ice_state

4.31.1 init thermo - setup salinity profile and tmelt for each layer

INTERFACE:

subroutine init_thermo

DESCRIPTION:

Setup the salinity profile and the melting temperature for each layer REVISION HISTORY:

author: C.M.Bitz

USES:

use ice_itd
use shr_sys_mod, only : shr_sys_abort

INPUT/OUTPUT PARAMETERS:

4.31.2 thermo vertical - heat budget over open water and ice

INTERFACE:

 subroutine thermo_vertical(i,j,hin,hsn,tiz,Fbot,
& dhi1,dhin,dhsn,hfatm,hfocn,qin)

DESCRIPTION:

Heat budget over open water and ice NOTE the wind stress is also computed here for later use

REVISION HISTORY:

author: C.M.Bitz

USES:

use ice_flux
use ice_albedo
use ice_atmo
use ice_history
use ice_calendar
use ice_itd
use ice_dh
use ice_tstm

INPUT/OUTPUT PARAMETERS:

 integer (kind=int_kind), intent(in) :: i, j
 real (kind=dbl_kind), intent(in) ::
& Fbot

 real (kind=dbl_kind), intent(inout) ::
& hin(ncat) ! ice thickness for each cat (m)
&, hsn(ncat) ! snow thickness for each cat (m)
&, tiz(0:nmax,ncat) ! temp of each layer for each cat (C)

 real (kind=dbl_kind), intent(out) ::
& dhi1 ! melt at bottom and top plus sublimation (m)
&, dhin(ncat) ! ice thickness change (m)
&, dhsn(ncat) ! snow thickness change (m)
&, hfatm ! heat flx to ice-snow from atm (J/m**2)
&, hfocn ! heat flx to ice-snow from ocn (J/m**2)
&, qin(nmax,ncat) ! enthalpy per unit volume (J/m**3)

5 Making Modifications to Code

There are three general types of code modifications one can consider: (1) adding further diagnostics but not changing the bit-for-bit answers, (2) answer changing modifications to the code by way of changing algorithms, and (3) adding prognostic variables. The first can be as simple as adding new fields to the history file, or producing more diagnostics to the existing code. The second can involve many conceivable changes in the physical algorithms of the sea ice model. The third is the most complex, with the most far-reaching of effects. Each of these will be touched on here, to give the user some indication how to proceed.

Modifications to the sea ice model involve either (or both) modifying existing code and possible additions of new modules. It is strongly recommended that in either case, modifications follow the same general code structure as in the existing code; in particular, using the protex keywords for documentation. New code which adheres to the existing conventions will be more likely to be accepted for inclusion in future releases of CSIM.

5.1 Adding Fields to the History File

The user may add fields to the history file, as follows. The parameter for the number of fields (avgsiz) must be increased accordingly (see module ice history), the desired field(s) stored internally in the accumulator array (aa), the field name, units and description specified in data statements in the netCDF write routine (ice write hist), and finally the field(s) included in the appropriate input parameter file. Once these field(s) are added, the standard option to enable/disable history tape fields applies (see the CSIM User’s Guide Version 4 for more information).

5.2 Changing Algorithms

The main pitfall in doing this is to be aware of what the coupler and the other CCSM components expect from the ice model. Any changes that effect the coupler exchange, in terms of definitions of fields or even adding/subtracting fields is not recommended. It is best to leave alone the coupler exchange fields when modifying algorithms unless it is crucial for the new algorithm. This would then requre major modifications to the coupler and/or other components, all of which is beyond the scope of this document.

5.3 Adding Prognostic Fields

Adding a new prognostic should not be too difficult. The prognostic can be either category dependent or not. Placing the new field in the module ice state in a manner consistent with the existing prognostics will ensure its availability in existing modules. Careful consideration should be given to where the new prognostic will be updated in the time stepping in the driver file ice.F . It might be wise to add the prognostic to the history file for output. It is necessary to add the new prognostic to the restart file if the exact restart character of the sea ice model is to be maintained (crucial for coupled model integrations). It might be wise to test the new prognostic in Active Ice Only (AIO) runs first, before attempting to run fully or partially coupled to other components.

5.4 Modifying Restart Files

Restart file writes and reads can be found in the module ice history. The structure of the restart files can be surmised from the writes and reads in the routines dumpfile and restartfile respectively. One needs to determine where in the time sequencing the appropriate restart field(s) need(s) to be assigned, and then written by adding extrae write code in dumpfile, as well as read code in restartfile. Exact restarts can be checked by running a startup run more than two days, rerunning but stopping at least one day short of the first run, and then restarting. The diagnostic log file printout from the sea ice model at the end of the first and the latter two runs should be identical. This ensures bit-for-bit restartability.

6 Miscellaneous Features

The sea ice model has standard diagnostic printout which can be modified. For any such modifications, as well as for those which change the actual simulation, care must be taken not to alter existing budget checks, in particular water and energy. These are briefly discussed here. The diagnostic printout code is found in module ice diagnostics.

6.1 Diagnostic Printouts

Diagnostic output to the log files consists of instantaneous hemispheric mean fields at a user selected frequency. Included is the model step number, the date (yyyymmdd, where yyyy is the year, mm the month, and dd the day), along with the renormalization factors for the conservation of ice after minimum values are removed. Then come a list of fields with max values (max cH) and hemispheric area weighted (arwt) values. The frequency of diagnostic output can be varied: see the CSIM User’s Guide Version 4.

6.2 Water and Energy Budgets

Various terms in the water budget are gathered in the routine runtime diags in the module ice diagnostics. Hemispherice (northern and southern) area weighted sums are performed. Modifying the code may require modifying the budget calculation to ensure all terms are included.

7 Summary

This CSIM Code Reference Manual Version 4 gives a brief overview as well as a detailed code listing. It gives suggesions on how to modify the existing code. It should be useful as a starting point and reference for anyone wishing to work with the CSIM source code.

References

Briegleb, B. P., C. M. Bitz, E. C. Hunke, W. H. Lipscomb and J. L. Schramm, 2002: Description of the Community Climate

System Model Version 2 Sea Ice Model. National Center for Atmospheric Research, http://www.cesm.ucar.edu/models/icecsim4.

Schramm, J. L., 2002: Community Sea Ice Model (CSIM) User’s Guide Version 4.0. National Center for Atmospheric Research,

http://www.cesm.ucar.edu/models/ice-csim4.